{"text_format":"1","workbook":"xlsx","n_sheets":8,"sheets":["各层参数","参数","设备地址","设备0","设备1","设备2","设备3","设备4"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"各层参数","index":0,"n_rows":116,"n_cols":11,"rows_kept":116,"cut":false,"hidden":false,"merged":[]}
["界面","描述","属性名","类型","放大","可写","A层HMI寄存器","B层HMI寄存器","C层HMI寄存器","D层HMI寄存器","E层HMI寄存器"]
["主界面","报警开关","AlarmIsOn","bool",null,"Y","设备1_读写M0970","设备0_读写M0970","设备2_读写M0970","设备3_读写M0970","设备4_读写M0970"]
["主界面","报警复位","IsAlarmReseted","bool",null,"Y","设备1_读写M0971","设备0_读写M0971","设备2_读写M0971","设备3_读写M0971","设备4_读写M0971"]
["主界面","累计产量","CumulativeProduction","float",null,null,"设备1_读写D6320","设备0_读写D6320","设备2_读写D6320","设备3_读写D6320","设备4_读写D6320"]
["主界面","配料斗重量显示","MixBucketWeight","float",null,null,"设备1_读写D184","设备0_读写D184","设备2_读写D184","设备3_读写D184","设备4_读写D184"]
["主界面","配料斗阀门","BucketValveIsOpen","bool",null,"Y","设备1_读写M0020","设备0_读写M0020","设备2_读写M0020","设备3_读写M0020","设备4_读写M0020"]
["主界面","配料操作","MixIsOn","bool",null,"Y","设备1_读写M0035","设备0_读写M0035","设备2_读写M0035","设备3_读写M0035","设备4_读写M0035"]
["主界面","失重仓重量","BinWeight","Int32",0.001,null,"设备1_读写D160","设备0_读写D160","设备2_读写D160","设备3_读写D160","设备4_读写D160"]
["主界面","当前产量","CurrentFlow","UInt16",0.1,null,"设备1_读写D2398","设备0_读写D2398","设备2_读写D2398","设备3_读写D2398","设备4_读写D2398"]
["主界面","设定产量","FlowSetting","UInt16",0.1,null,"设备1_读写D2144","设备0_读写D2144","设备2_读写D2144","设备3_读写D2144","设备4_读写D2144"]
["主界面","运行比例","ScrewPDisp","UInt16",0.1,null,"设备1_读写D3702","设备1_读写D3704","设备1_读写D3706","设备1_读写D3710","设备1_读写D3712"]
["主界面","设定比例","ScrewPSet","UInt16",0.1,"Y","设备1_读写D3802","设备1_读写D3804","设备1_读写D3806","设备1_读写D3830","设备1_读写D3832"]
["主界面","运行频率","ScrewMotorFreq","UInt16",0.1,null,"设备1_读写D2320","设备0_读写D2320","设备2_读写D2320","设备3_读写D2320","设备4_读写D2320"]
["主界面","设定频率","ScrewManualFreq","UInt16",0.1,"Y","设备1_读写D2308","设备0_读写D2308","设备2_读写D2308","设备3_读写D2308","设备4_读写D2308"]
["主界面","设定频率确定","ScrewManualFreqIsSet","bool",null,"Y","设备1_读写M0350","设备0_读写M0350","设备2_读写M0350","设备3_读写M0350","设备4_读写M0350"]
["主界面","螺杆模式","ScrewIsAutoMode","bool",null,"Y","设备1_读写M0910","设备0_读写M0910","设备2_读写M0910","设备3_读写M0910","设备4_读写M0910"]
["主界面","螺杆操作","ScrewMotorIsOn","bool",null,"Y","设备1_读写M0150","设备0_读写M0150","设备2_读写M0150","设备3_读写M0150","设备4_读写M0150"]
["配置画面","配料数据保存","IsMixSave","bool",null,null,"设备1_读写M0490","设备0_读写M0490","设备2_读写M0490","设备3_读写M0490","设备4_读写M0490"]
["配置画面","1#比例设定","MixPSet_1","UInt16",0.1,"Y","设备1_读写D1000","设备0_读写D1000","设备2_读写D1000","设备3_读写D1000","设备4_读写D1000"]
["配置画面","2#比例设定","MixPSet_2","UInt16",0.1,"Y","设备1_读写D1001","设备0_读写D1001","设备2_读写D1001","设备3_读写D1001","设备4_读写D1001"]
["配置画面","3#比例设定","MixPSet_3","UInt16",0.1,"Y","设备1_读写D1002","设备0_读写D1002","设备2_读写D1002","设备3_读写D1002","设备4_读写D1002"]
["配置画面","4#比例设定","MixPSet_4","UInt16",0.1,"Y","设备1_读写D1003","设备0_读写D1003","设备2_读写D1003","设备3_读写D1003","设备4_读写D1003"]
["配置画面","1#比例显示","MixPDisp_1","float",null,null,"设备1_读写D6304","设备0_读写D6304","设备2_读写D6304","设备3_读写D6304","设备4_读写D6304"]
["配置画面","2#比例显示","MixPDisp_2","float",null,null,"设备1_读写D6308","设备0_读写D6308","设备2_读写D6308","设备3_读写D6308","设备4_读写D6308"]
["配置画面","3#比例显示","MixPDisp_3","float",null,null,"设备1_读写D6312","设备0_读写D6312","设备2_读写D6312","设备3_读写D6312","设备4_读写D6312"]
["配置画面","4#比例显示","MixPDisp_4","float",null,null,"设备1_读写D6316","设备0_读写D6316","设备2_读写D6316","设备3_读写D6316","设备4_读写D6316"]
["配置画面","1#重量设定","MixSet_1","float",null,null,"设备1_读写D6080","设备0_读写D6080","设备2_读写D6080","设备3_读写D6080","设备4_读写D6080"]
["配置画面","2#重量设定","MixSet_2","float",null,null,"设备1_读写D5080","设备0_读写D5080","设备2_读写D5080","设备3_读写D5080","设备4_读写D5080"]
["配置画面","3#重量设定","MixSet_3","float",null,null,"设备1_读写D4080","设备0_读写D4080","设备2_读写D4080","设备3_读写D4080","设备4_读写D4080"]
["配置画面","4#重量设定","MixSet_4","float",null,null,"设备1_读写D3080","设备0_读写D3080","设备2_读写D3080","设备3_读写D3080","设备4_读写D3080"]
["配置画面","1#重量显示","MixDisp_1","float",null,null,"设备1_读写D6084","设备0_读写D6084","设备2_读写D6084","设备3_读写D6084","设备4_读写D6084"]
["配置画面","2#重量显示","MixDisp_2","float",null,null,"设备1_读写D5084","设备0_读写D5084","设备2_读写D5084","设备3_读写D5084","设备4_读写D5084"]
["配置画面","3#重量显示","MixDisp_3","float",null,null,"设备1_读写D4084","设备0_读写D4084","设备2_读写D4084","设备3_读写D4084","设备4_读写D4084"]
["配置画面","4#重量显示","MixDisp_4","float",null,null,"设备1_读写D3084","设备0_读写D3084","设备2_读写D3084","设备3_读写D3084","设备4_读写D3084"]
["配置画面","1#放料","MixLight_1","bool",null,null,"设备1_读写Y0001","设备0_读写Y0001","设备2_读写Y0001","设备3_读写Y0001","设备4_读写Y0001"]
["配置画面","2#放料","MixLight_2","bool",null,null,"设备1_读写Y0002","设备0_读写Y0002","设备2_读写Y0002","设备3_读写Y0002","设备4_读写Y0002"]
["配置画面","3#放料","MixLight_3","bool",null,null,"设备1_读写Y0003","设备0_读写Y0003","设备2_读写Y0003","设备3_读写Y0003","设备4_读写Y0003"]
["配置画面","4#放料","MixLight_4","bool",null,null,"设备1_读写Y0004","设备0_读写Y0004","设备2_读写Y0004","设备3_读写Y0004","设备4_读写Y0004"]
["配置画面","配料斗卸载","MixUnload","bool",null,null,"设备1_读写Y0005","设备0_读写Y0005","设备2_读写Y0005","设备3_读写Y0005","设备4_读写Y0005"]
["配置画面","配料斗重量设置","MixSet","float",null,"Y","设备1_读写D6012","设备0_读写D6012","设备2_读写D6012","设备3_读写D6012","设备4_读写D6012"]
["配置画面","配料斗重量显示","MixDisp","float",null,null,"设备1_读写D6300","设备0_读写D6300","设备2_读写D6300","设备3_读写D6300","设备4_读写D6300"]
["配置画面","1#累计重量","MixCum_1","float",null,null,"设备1_读写D6322","设备0_读写D6322","设备2_读写D6322","设备3_读写D6322","设备4_读写D6322"]
["配置画面","2#累计重量","MixCum_2","float",null,null,"设备1_读写D6326","设备0_读写D6326","设备2_读写D6326","设备3_读写D6326","设备4_读写D6326"]
["配置画面","3#累计重量","MixCum_3","float",null,null,"设备1_读写D6330","设备0_读写D6330","设备2_读写D6330","设备3_读写D6330","设备4_读写D6330"]
["配置画面","4#累计重量","MixCum_4","float",null,null,"设备1_读写D6334","设备0_读写D6334","设备2_读写D6334","设备3_读写D6334","设备4_读写D6334"]
["配置画面","1#累计百分比","MixCumPercent_1","float",null,null,"设备1_读写D6324","设备0_读写D6324","设备2_读写D6324","设备3_读写D6324","设备4_读写D6324"]
["配置画面","2#累计百分比","MixCumPercent_2","float",null,null,"设备1_读写D6328","设备0_读写D6328","设备2_读写D6328","设备3_读写D6328","设备4_读写D6328"]
["配置画面","3#累计百分比","MixCumPercent_3","float",null,null,"设备1_读写D6332","设备0_读写D6332","设备2_读写D6332","设备3_读写D6332","设备4_读写D6332"]
["配置画面","4#累计百分比","MixCumPercent_4","float",null,null,"设备1_读写D6336","设备0_读写D6336","设备2_读写D6336","设备3_读写D6336","设备4_读写D6336"]
["配置画面","产量清零","ClearProduction","bool",null,"Y","设备1_读写M0156","设备0_读写M0156","设备2_读写M0156","设备3_读写M0156","设备4_读写M0156"]
["螺杆参数","流量方式","FlowCalMethodIsA","bool",null,"Y","设备1_读写M3000","设备0_读写M3000","设备2_读写M3000","设备3_读写M3000","设备4_读写M3000"]
["螺杆参数","流量反馈","FlowDisp","UInt16",0.1,null,"设备1_读写D2170","设备0_读写D2170","设备2_读写D2170","设备3_读写D2170","设备4_读写D2170"]
["螺杆参数","滤波系数设定","FilterParam","UInt16",0.1,"Y","设备1_读写D2002","设备0_读写D2002","设备2_读写D2002","设备3_读写D2002","设备4_读写D2002"]
["螺杆参数","切换级别设定","SwitchLv","UInt16",0.1,"Y","设备1_读写D2610","设备0_读写D2610","设备2_读写D2610","设备3_读写D2610","设备4_读写D2610"]
["螺杆参数","升降增益设定","UpDownGain","UInt16",0.01,"Y","设备1_读写D2040","设备0_读写D2040","设备2_读写D2040","设备3_读写D2040","设备4_读写D2040"]
["螺杆参数","比例增益设定","PGain","UInt16",0.01,"Y","设备1_读写D2034","设备0_读写D2034","设备2_读写D2034","设备3_读写D2034","设备4_读写D2034"]
["螺杆参数","积分时间设定","ITime","UInt16",null,"Y","设备1_读写D2004","设备0_读写D2004","设备2_读写D2004","设备3_读写D2004","设备4_读写D2004"]
["螺杆参数","调节系数设定","AdjustFactor","UInt16",0.01,"Y","设备1_读写D2050","设备0_读写D2050","设备2_读写D2050","设备3_读写D2050","设备4_读写D2050"]
["螺杆参数","调节上限设定","AdjustUpper","Int16",null,"Y","设备1_读写D2022","设备0_读写D2022","设备2_读写D2022","设备3_读写D2022","设备4_读写D2022"]
["螺杆参数","调节下限设定","AdjustLower","Int16",null,"Y","设备1_读写D2023","设备0_读写D2023","设备2_读写D2023","设备3_读写D2023","设备4_读写D2023"]
["螺杆参数","稳定级别切换","StableLvSwitch","UInt16",0.1,"Y","设备1_读写D2662","设备0_读写D2662","设备2_读写D2662","设备3_读写D2662","设备4_读写D2662"]
["螺杆参数","PID调节限幅","PIDLimit","UInt16",null,"Y","设备1_读写D2762","设备0_读写D2762","设备2_读写D2762","设备3_读写D2762","设备4_读写D2762"]
["螺杆参数","采样时间","SampleTime","UInt16",null,null,"设备1_读写D2000","设备0_读写D2000","设备2_读写D2000","设备3_读写D2000","设备4_读写D2000"]
["螺杆参数","PID结果","PIDResult","Int16",null,null,"设备1_读写D2030","设备0_读写D2030","设备2_读写D2030","设备3_读写D2030","设备4_读写D2030"]
["螺杆参数","PID调节","PIDAdjust","Int16",null,null,"设备1_读写D2058","设备0_读写D2058","设备2_读写D2058","设备3_读写D2058","设备4_读写D2058"]
["螺杆参数","实际速度","ScrewCurrentSpeed","UInt16",null,null,"设备1_读写D2700","设备0_读写D2700","设备2_读写D2700","设备3_读写D2700","设备4_读写D2700"]
["螺杆参数","比例增益","PGainDisp","UInt16",0.01,null,"设备1_读写D2003","设备0_读写D2003","设备2_读写D2003","设备3_读写D2003","设备4_读写D2003"]
["参数设置","卸料时间","UnloadingTime","UInt16",0.1,"Y","设备1_读写D2520","设备0_读写D2520","设备2_读写D2520","设备3_读写D2520","设备4_读写D2520"]
["参数设置","零位稳定时间","ZeroStableTime","UInt16",0.1,"Y","设备1_读写D2521","设备0_读写D2521","设备2_读写D2521","设备3_读写D2521","设备4_读写D2521"]
["参数设置","流量切换允许","FlowSwitchEnable","UInt16",0.1,"Y","设备1_读写D2374","设备0_读写D2374","设备2_读写D2374","设备3_读写D2374","设备4_读写D2374"]
["参数设置","取样时间设定(s)","SampleTimeSet","UInt16",0.1,"Y","设备1_读写D2132","设备0_读写D2132","设备2_读写D2132","设备3_读写D2132","设备4_读写D2132"]
["参数设置","额定频率(Hz)","ScrewMotorRatedFreq","UInt16",0.1,"Y","设备1_读写D2324","设备0_读写D2324","设备2_读写D2324","设备3_读写D2324","设备4_读写D2324"]
["参数设置","重量稳定时间(s)","WeightStableTime","UInt16",0.1,"Y","设备1_读写D1184","设备0_读写D1184","设备2_读写D1184","设备3_读写D1184","设备4_读写D1184"]
["参数设置","料位下限设定(kg)","MaterialLowLimitSet","UInt16",0.1,"Y","设备1_读写D2182","设备0_读写D2182","设备2_读写D2182","设备3_读写D2182","设备4_读写D2182"]
["参数设置","报警偏差设定(%)","AlarmDeviationSet","UInt16",null,"Y","设备1_读写D2140","设备0_读写D2140","设备2_读写D2140","设备3_读写D2140","设备4_读写D2140"]
["参数设置","重量校正系数","WeightCorrectFactor","UInt16",0.01,"Y","设备1_读写D2620","设备0_读写D2620","设备2_读写D2620","设备3_读写D2620","设备4_读写D2620"]
["参数设置","缺料报警设定(kg)","LackErrorSet","UInt16",0.1,"Y","设备1_读写D2184","设备0_读写D2184","设备2_读写D2184","设备3_读写D2184","设备4_读写D2184"]
["参数设置","搅拌时间设定(s)","MixingTimeSet","UInt16",0.1,"Y","设备1_读写D3680","设备0_读写D3680","设备2_读写D3680","设备3_读写D3680","设备4_读写D3680"]
["配料参数","1次补料偏差","FeedingDeviation_1","float",null,"Y","设备1_读写D2510","设备0_读写D2510","设备2_读写D2510","设备3_读写D2510","设备4_读写D2510"]
["配料参数","2次补料偏差","FeedingDeviation_2","float",null,"Y","设备1_读写D2512","设备0_读写D2512","设备2_读写D2512","设备3_读写D2512","设备4_读写D2512"]
["配料参数","3次补料偏差","FeedingDeviation_3","float",null,"Y","设备1_读写D2514","设备0_读写D2514","设备2_读写D2514","设备3_读写D2514","设备4_读写D2514"]
["配料参数","4次补料偏差","FeedingDeviation_4","float",null,"Y","设备1_读写D2516","设备0_读写D2516","设备2_读写D2516","设备3_读写D2516","设备4_读写D2516"]
["配料参数","1次加料设定","FeedSet_1","float",null,"Y","设备1_读写D6026","设备0_读写D6026","设备2_读写D6026","设备3_读写D6026","设备4_读写D6026"]
["配料参数","2次加料设定","FeedSet_2","float",null,"Y","设备1_读写D5026","设备0_读写D5026","设备2_读写D5026","设备3_读写D5026","设备4_读写D5026"]
["配料参数","3次加料设定","FeedSet_3","float",null,"Y","设备1_读写D4026","设备0_读写D4026","设备2_读写D4026","设备3_读写D4026","设备4_读写D4026"]
["配料参数","4次加料设定","FeedSet_4","float",null,"Y","设备1_读写D3026","设备0_读写D3026","设备2_读写D3026","设备3_读写D3026","设备4_读写D3026"]
["配料参数","1#初始时间","InitTime_1","UInt16",0.1,"Y","设备1_读写D2500","设备0_读写D2500","设备2_读写D2500","设备3_读写D2500","设备4_读写D2500"]
["配料参数","2#初始时间","InitTime_2","UInt16",0.1,"Y","设备1_读写D2501","设备0_读写D2501","设备2_读写D2501","设备3_读写D2501","设备4_读写D2501"]
["配料参数","3#初始时间","InitTime_3","UInt16",0.1,"Y","设备1_读写D2502","设备0_读写D2502","设备2_读写D2502","设备3_读写D2502","设备4_读写D2502"]
["配料参数","4#初始时间","InitTime_4","UInt16",0.1,"Y","设备1_读写D2503","设备0_读写D2503","设备2_读写D2503","设备3_读写D2503","设备4_读写D2503"]
["配料参数","1#最小时间","MinTime_1","UInt16",0.001,"Y","设备1_读写D6090","设备0_读写D6090","设备2_读写D6090","设备3_读写D6090","设备4_读写D6090"]
["配料参数","2#最小时间","MinTime_2","UInt16",0.001,"Y","设备1_读写D5090","设备0_读写D5090","设备2_读写D5090","设备3_读写D5090","设备4_读写D5090"]
["配料参数","3#最小时间","MinTime_3","UInt16",0.001,"Y","设备1_读写D4090","设备0_读写D4090","设备2_读写D4090","设备3_读写D4090","设备4_读写D4090"]
["配料参数","4#最小时间","MinTime_4","UInt16",0.001,"Y","设备1_读写D3090","设备0_读写D3090","设备2_读写D3090","设备3_读写D3090","设备4_读写D3090"]
["配料参数","1#稳重时间","StableTime_1","UInt16",0.1,"Y","设备1_读写D2504","设备0_读写D2504","设备2_读写D2504","设备3_读写D2504","设备4_读写D2504"]
["配料参数","2#稳重时间","StableTime_2","UInt16",0.1,"Y","设备1_读写D2505","设备0_读写D2505","设备2_读写D2505","设备3_读写D2505","设备4_读写D2505"]
["配料参数","3#稳重时间","StableTime_3","UInt16",0.1,"Y","设备1_读写D2506","设备0_读写D2506","设备2_读写D2506","设备3_读写D2506","设备4_读写D2506"]
["配料参数","4#稳重时间","StableTime_4","UInt16",0.1,"Y","设备1_读写D2507","设备0_读写D2507","设备2_读写D2507","设备3_读写D2507","设备4_读写D2507"]
["配料参数","1次料仓报警设定","BinAlarmSet_1","UInt16",null,"Y","设备1_读写D3580","设备0_读写D3580","设备2_读写D3580","设备3_读写D3580","设备4_读写D3580"]
["配料参数","2次料仓报警设定","BinAlarmSet_2","UInt16",null,"Y","设备1_读写D3582","设备0_读写D3582","设备2_读写D3582","设备3_读写D3582","设备4_读写D3582"]
["配料参数","3次料仓报警设定","BinAlarmSet_3","UInt16",null,"Y","设备1_读写D3584","设备0_读写D3584","设备2_读写D3584","设备3_读写D3584","设备4_读写D3584"]
["配料参数","4次料仓报警设定","BinAlarmSet_4","UInt16",null,"Y","设备1_读写D3586","设备0_读写D3586","设备2_读写D3586","设备3_读写D3586","设备4_读写D3586"]
["报警","No.1料仓缺料报警","IsErrorOfLack_1","bool",null,null,"设备1_读写M0500","设备0_读写M0500","设备2_读写M0500","设备3_读写M0500","设备4_读写M0500"]
["报警","No.2料仓缺料报警","IsErrorOfLack_2","bool",null,null,"设备1_读写M0501","设备0_读写M0501","设备2_读写M0501","设备3_读写M0501","设备4_读写M0501"]
["报警","No.3料仓缺料报警","IsErrorOfLack_3","bool",null,null,"设备1_读写M0502","设备0_读写M0502","设备2_读写M0502","设备3_读写M0502","设备4_读写M0502"]
["报警","No.4料仓缺料报警","IsErrorOfLack_4","bool",null,null,"设备1_读写M0503","设备0_读写M0503","设备2_读写M0503","设备3_读写M0503","设备4_读写M0503"]
["报警","No.1料斗加料异常","IsErrorOfAdd_1","bool",null,null,"设备1_读写M0510","设备0_读写M0510","设备2_读写M0510","设备3_读写M0510","设备4_读写M0510"]
["报警","No.2料斗加料异常","IsErrorOfAdd_2","bool",null,null,"设备1_读写M0511","设备0_读写M0511","设备2_读写M0511","设备3_读写M0511","设备4_读写M0511"]
["报警","No.3料斗加料异常","IsErrorOfAdd_3","bool",null,null,"设备1_读写M0512","设备0_读写M0512","设备2_读写M0512","设备3_读写M0512","设备4_读写M0512"]
["报警","No.4料斗加料异常","IsErrorOfAdd_4","bool",null,null,"设备1_读写M0513","设备0_读写M0513","设备2_读写M0513","设备3_读写M0513","设备4_读写M0513"]
["报警","螺杆缺料报警","IsErrorOfScrewLack","bool",null,null,"设备1_读写M0681","设备0_读写M0681","设备2_读写M0681","设备3_读写M0681","设备4_读写M0681"]
["报警","螺杆流量超偏差报警","IsErrorOfScrewFlow","bool",null,null,"设备1_读写M0684","设备0_读写M0684","设备2_读写M0684","设备3_读写M0684","设备4_读写M0684"]
["报警","搅拌电机故障","IsErrorOfBlender","bool",null,null,"设备1_只读X0002","设备0_只读X0002","设备2_只读X0002","设备3_只读X0002","设备4_只读X0002"]
["报警","急停开启","IsErrorOfScram","bool",null,null,"设备1_只读X0003","设备0_只读X0003","设备2_只读X0003","设备3_只读X0003","设备4_只读X0003"]
["报警","搅拌电机急停开启","IsErrorOfBlender2","bool",null,null,"设备1_只读X0004","设备0_只读X0004","设备2_只读X0004","设备3_只读X0004","设备4_只读X0004"]
["报警","搅拌电机未启动","IsErrorOfBlender3","bool",null,null,"设备1_读写M1300","设备0_读写M1300","设备2_读写M1300","设备3_读写M1300","设备4_读写M1300"]

{"sheet":"参数","index":1,"n_rows":25,"n_cols":7,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
["界面","描述","属性名","类型","放大","可写","HMI寄存器"]
["主界面","总流量设定","TotalFlowSetting","UInt16",0.1,"Y","设备1_读写D3800"]
["主界面","总流量显示","TotalFlow","UInt16",0.1,null,"设备1_读写D3700"]
["主界面","总产量","TotalProduction","float",null,null,"设备1_读写D600"]
["主界面","码轮周长mm","WheelPerimeter","float",null,"Y","设备1_读写R1014"]
["主界面","码轮脉冲","WheelPulse","float",null,"Y","设备1_读写R1016"]
["主界面","平均密度","Density","float",null,"Y","设备1_读写R1032"]
["主界面","边料不回收","IsRimNoRecycle","bool",null,"Y","设备1_读写M0003"]
["主界面","边料kg/h","RimCharge","float",null,null,"设备1_读写R1308"]
["主界面","厚度um","Thickness","float",null,null,"设备1_读写R1040"]
["主界面","当前线速度m/min","CurrentVelocity","float",null,null,"设备1_读写R1050"]
["主界面","当前线速度设置m/min","CurrentVelocitySet","UInt16",0.1,"Y","设备1_读写R1700"]
["主界面","吹膜宽度mm","TotalFilmWidth","float",null,"Y","设备1_读写R1030"]
["主界面","切边mm","RimWidth","float",null,"Y","设备1_读写R1204"]
["主界面","收卷宽度mm","ActFilmWidth","float",null,null,"设备1_读写R1206"]
["主界面","设定厚度um","SetThickness","float",null,"Y","设备1_读写R1106"]
["主界面","理论速度m/min","TargetVelocity","float",null,null,"设备1_读写R1126"]
["主界面","内收卷当前m","ACurrentLen","float",null,null,"设备1_读写R1352"]
["主界面","内收卷当前kg","ACurrent","float",null,null,"设备1_读写R1236"]
["主界面","内收卷上卷kg","ALast","float",null,null,"设备1_读写R1602"]
["主界面","外收卷当前m","BCurrentLen","float",null,null,"设备1_读写R1354"]
["主界面","外收卷当前kg","BCurrent","float",null,null,"设备1_读写R1226"]
["主界面","外收卷上卷kg","BLast","float",null,null,"设备1_读写R1600"]
["主界面","内收卷清零","AClear","bool",null,"Y","设备1_读写M0002"]
["主界面","外收卷清零","BClear","bool",null,"Y","设备1_读写M0001"]

{"sheet":"设备地址","index":2,"n_rows":6,"n_cols":2,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
["设备序号","EP"]
[0,"192.168.50.2:502"]
[1,"192.168.50.1:502"]
[2,"192.168.50.3:502"]
[3,"192.168.50.4:502"]
[4,"192.168.50.5:502"]

{"sheet":"设备0","index":3,"n_rows":145,"n_cols":8,"rows_kept":145,"cut":false,"hidden":false,"merged":[]}
["通道号","变量名","变量类型","通道名称","读写类型","寄存器名称","数据类型","寄存器地址"]
[1,"设备0_只读X0002","INTEGER","只读163491","只读","[1区]输入继电器","NULL",63491]
[2,"设备0_只读X0003","INTEGER","只读163492","只读","[1区]输入继电器","NULL",63492]
[3,"设备0_只读X0004","INTEGER","只读163493","只读","[1区]输入继电器","NULL",63493]
[4,"设备0_读写M0000","INTEGER","读写00001","读写","[0区]输出继电器","NULL",1]
[5,"设备0_读写M0020","INTEGER","读写00021","读写","[0区]输出继电器","NULL",21]
[6,"设备0_读写M0035","INTEGER","读写00036","读写","[0区]输出继电器","NULL",36]
[7,"设备0_读写M0150","INTEGER","读写00151","读写","[0区]输出继电器","NULL",151]
[8,"设备0_读写M0156","INTEGER","读写00157","读写","[0区]输出继电器","NULL",157]
[9,"设备0_读写M0350","INTEGER","读写00351","读写","[0区]输出继电器","NULL",351]
[10,"设备0_读写M0490","INTEGER","读写00491","读写","[0区]输出继电器","NULL",491]
[11,"设备0_读写M0500","INTEGER","读写00501","读写","[0区]输出继电器","NULL",501]
[12,"设备0_读写M0501","INTEGER","读写00502","读写","[0区]输出继电器","NULL",502]
[13,"设备0_读写M0502","INTEGER","读写00503","读写","[0区]输出继电器","NULL",503]
[14,"设备0_读写M0503","INTEGER","读写00504","读写","[0区]输出继电器","NULL",504]
[15,"设备0_读写M0510","INTEGER","读写00511","读写","[0区]输出继电器","NULL",511]
[16,"设备0_读写M0511","INTEGER","读写00512","读写","[0区]输出继电器","NULL",512]
[17,"设备0_读写M0512","INTEGER","读写00513","读写","[0区]输出继电器","NULL",513]
[18,"设备0_读写M0513","INTEGER","读写00514","读写","[0区]输出继电器","NULL",514]
[19,"设备0_读写M0540","INTEGER","读写00541","读写","[0区]输出继电器","NULL",541]
[20,"设备0_读写M0681","INTEGER","读写00682","读写","[0区]输出继电器","NULL",682]
[21,"设备0_读写M0684","INTEGER","读写00685","读写","[0区]输出继电器","NULL",685]
[22,"设备0_读写M0910","INTEGER","读写00911","读写","[0区]输出继电器","NULL",911]
[23,"设备0_读写M0920","INTEGER","读写00921","读写","[0区]输出继电器","NULL",921]
[24,"设备0_读写M927","INTEGER","读写00927","读写","[0区]输出继电器","NULL",927]
[25,"设备0_读写M0950","INTEGER","读写00951","读写","[0区]输出继电器","NULL",951]
[26,"设备0_读写M0951","INTEGER","读写00952","读写","[0区]输出继电器","NULL",952]
[27,"设备0_读写M0952","INTEGER","读写00953","读写","[0区]输出继电器","NULL",953]
[28,"设备0_读写M0953","INTEGER","读写00954","读写","[0区]输出继电器","NULL",954]
[29,"设备0_读写M0954","INTEGER","读写00955","读写","[0区]输出继电器","NULL",955]
[30,"设备0_读写M0955","INTEGER","读写00956","读写","[0区]输出继电器","NULL",956]
[31,"设备0_读写M0956","INTEGER","读写00957","读写","[0区]输出继电器","NULL",957]
[32,"设备0_读写M0957","INTEGER","读写00958","读写","[0区]输出继电器","NULL",958]
[33,"设备0_读写M0958","INTEGER","读写00959","读写","[0区]输出继电器","NULL",959]
[34,"设备0_读写M0959","INTEGER","读写00960","读写","[0区]输出继电器","NULL",960]
[35,"设备0_读写M0960","INTEGER","读写00961","读写","[0区]输出继电器","NULL",961]
[36,"设备0_读写M0961","INTEGER","读写00962","读写","[0区]输出继电器","NULL",962]
[37,"设备0_读写M0963","INTEGER","读写00964","读写","[0区]输出继电器","NULL",964]
[38,"设备0_读写M0964","INTEGER","读写00965","读写","[0区]输出继电器","NULL",965]
[39,"设备0_读写M0965","INTEGER","读写00966","读写","[0区]输出继电器","NULL",966]
[40,"设备0_读写M0966","INTEGER","读写00967","读写","[0区]输出继电器","NULL",967]
[41,"设备0_读写M0967","INTEGER","读写00968","读写","[0区]输出继电器","NULL",968]
[42,"设备0_读写M0968","INTEGER","读写00969","读写","[0区]输出继电器","NULL",969]
[43,"设备0_读写M0970","INTEGER","读写00971","读写","[0区]输出继电器","NULL",971]
[44,"设备0_读写M0971","INTEGER","读写00972","读写","[0区]输出继电器","NULL",972]
[45,"设备0_读写M1300","INTEGER","读写01301","读写","[0区]输出继电器","NULL",1301]
[46,"设备0_读写M3000","INTEGER","读写03001","读写","[0区]输出继电器","NULL",3001]
[47,"设备0_读写Y0001","INTEGER","读写064514","读写","[0区]输出继电器","NULL",64514]
[48,"设备0_读写Y0002","INTEGER","读写064515","读写","[0区]输出继电器","NULL",64515]
[49,"设备0_读写Y0003","INTEGER","读写064516","读写","[0区]输出继电器","NULL",64516]
[50,"设备0_读写Y0004","INTEGER","读写064517","读写","[0区]输出继电器","NULL",64517]
[51,"设备0_读写Y0005","INTEGER","读写064518","读写","[0区]输出继电器","NULL",64518]
[52,"设备0_读写D160","SINGLE","读写4DB0161","读写","[4区]输出寄存器","32位 有符号二进制",161]
[53,"设备0_读写D184","SINGLE","读写4DF0185","读写","[4区]输出寄存器","32位 浮点数",185]
[54,"设备0_读写D600","SINGLE","读写4DF0601","读写","[4区]输出寄存器","32位 浮点数",601]
[55,"设备0_读写D1000","SINGLE","读写4WUB1001","读写","[4区]输出寄存器","16位 无符号二进制",1001]
[56,"设备0_读写D1001","SINGLE","读写4WUB1002","读写","[4区]输出寄存器","16位 无符号二进制",1002]
[57,"设备0_读写D1002","SINGLE","读写4WUB1003","读写","[4区]输出寄存器","16位 无符号二进制",1003]
[58,"设备0_读写D1003","SINGLE","读写4WUB1004","读写","[4区]输出寄存器","16位 无符号二进制",1004]
[59,"设备0_读写D1184","SINGLE","读写4WUB1185","读写","[4区]输出寄存器","16位 无符号二进制",1185]
[60,"设备0_读写D2000","SINGLE","读写4WUB2001","读写","[4区]输出寄存器","16位 无符号二进制",2001]
[61,"设备0_读写D2002","SINGLE","读写4WUB2003","读写","[4区]输出寄存器","16位 无符号二进制",2003]
[62,"设备0_读写D2003","SINGLE","读写4WUB2004","读写","[4区]输出寄存器","16位 无符号二进制",2004]
[63,"设备0_读写D2004","SINGLE","读写4WUB2005","读写","[4区]输出寄存器","16位 无符号二进制",2005]
[64,"设备0_读写D2022","SINGLE","读写4WB2023","读写","[4区]输出寄存器","16位 有符号二进制",2023]
[65,"设备0_读写D2023","SINGLE","读写4WB2024","读写","[4区]输出寄存器","16位 有符号二进制",2024]
[66,"设备0_读写D2030","SINGLE","读写4WB2031","读写","[4区]输出寄存器","16位 有符号二进制",2031]
[67,"设备0_读写D2034","SINGLE","读写4WUB2035","读写","[4区]输出寄存器","16位 无符号二进制",2035]
[68,"设备0_读写D2040","SINGLE","读写4WUB2041","读写","[4区]输出寄存器","16位 无符号二进制",2041]
[69,"设备0_读写D2050","SINGLE","读写4WUB2051","读写","[4区]输出寄存器","16位 无符号二进制",2051]
[70,"设备0_读写D2058","SINGLE","读写4WB2059","读写","[4区]输出寄存器","16位 有符号二进制",2059]
[71,"设备0_读写D2132","SINGLE","读写4WUB2133","读写","[4区]输出寄存器","16位 无符号二进制",2133]
[72,"设备0_读写D2140","SINGLE","读写4WUB2141","读写","[4区]输出寄存器","16位 无符号二进制",2141]
[73,"设备0_读写D2144","SINGLE","读写4WUB2145","读写","[4区]输出寄存器","16位 无符号二进制",2145]
[74,"设备0_读写D2170","SINGLE","读写4WUB2171","读写","[4区]输出寄存器","16位 无符号二进制",2171]
[75,"设备0_读写D2182","SINGLE","读写4WUB2183","读写","[4区]输出寄存器","16位 无符号二进制",2183]
[76,"设备0_读写D2184","SINGLE","读写4WUB2185","读写","[4区]输出寄存器","16位 无符号二进制",2185]
[77,"设备0_读写D2308","SINGLE","读写4WUB2309","读写","[4区]输出寄存器","16位 无符号二进制",2309]
[78,"设备0_读写D2320","SINGLE","读写4WUB2321","读写","[4区]输出寄存器","16位 无符号二进制",2321]
[79,"设备0_读写D2324","SINGLE","读写4WUB2325","读写","[4区]输出寄存器","16位 无符号二进制",2325]
[80,"设备0_读写D2374","SINGLE","读写4WUB2375","读写","[4区]输出寄存器","16位 无符号二进制",2375]
[81,"设备0_读写D2398","SINGLE","读写4WUB2399","读写","[4区]输出寄存器","16位 无符号二进制",2399]
[82,"设备0_读写D2500","SINGLE","读写4WUB2501","读写","[4区]输出寄存器","16位 无符号二进制",2501]
[83,"设备0_读写D2501","SINGLE","读写4WUB2502","读写","[4区]输出寄存器","16位 无符号二进制",2502]
[84,"设备0_读写D2502","SINGLE","读写4WUB2503","读写","[4区]输出寄存器","16位 无符号二进制",2503]
[85,"设备0_读写D2503","SINGLE","读写4WUB2504","读写","[4区]输出寄存器","16位 无符号二进制",2504]
[86,"设备0_读写D2504","SINGLE","读写4WUB2505","读写","[4区]输出寄存器","16位 无符号二进制",2505]
[87,"设备0_读写D2505","SINGLE","读写4WUB2506","读写","[4区]输出寄存器","16位 无符号二进制",2506]
[88,"设备0_读写D2506","SINGLE","读写4WUB2507","读写","[4区]输出寄存器","16位 无符号二进制",2507]
[89,"设备0_读写D2507","SINGLE","读写4WUB2508","读写","[4区]输出寄存器","16位 无符号二进制",2508]
[90,"设备0_读写D2510","SINGLE","读写4DF2511","读写","[4区]输出寄存器","32位 浮点数",2511]
[91,"设备0_读写D2512","SINGLE","读写4DF2513","读写","[4区]输出寄存器","32位 浮点数",2513]
[92,"设备0_读写D2514","SINGLE","读写4DF2515","读写","[4区]输出寄存器","32位 浮点数",2515]
[93,"设备0_读写D2516","SINGLE","读写4DF2517","读写","[4区]输出寄存器","32位 浮点数",2517]
[94,"设备0_读写D2520","SINGLE","读写4WUB2521","读写","[4区]输出寄存器","16位 无符号二进制",2521]
[95,"设备0_读写D2521","SINGLE","读写4WUB2522","读写","[4区]输出寄存器","16位 无符号二进制",2522]
[96,"设备0_读写D2610","SINGLE","读写4WUB2611","读写","[4区]输出寄存器","16位 无符号二进制",2611]
[97,"设备0_读写D2620","SINGLE","读写4WUB2621","读写","[4区]输出寄存器","16位 无符号二进制",2621]
[98,"设备0_读写D2662","SINGLE","读写4WUB2663","读写","[4区]输出寄存器","16位 无符号二进制",2663]
[99,"设备0_读写D2700","SINGLE","读写4WUB2701","读写","[4区]输出寄存器","16位 无符号二进制",2701]
[100,"设备0_读写D2762","SINGLE","读写4WUB2763","读写","[4区]输出寄存器","16位 无符号二进制",2763]
[101,"设备0_读写D3026","SINGLE","读写4DF3027","读写","[4区]输出寄存器","32位 浮点数",3027]
[102,"设备0_读写D3080","SINGLE","读写4DF3081","读写","[4区]输出寄存器","32位 浮点数",3081]
[103,"设备0_读写D3084","SINGLE","读写4DF3085","读写","[4区]输出寄存器","32位 浮点数",3085]
[104,"设备0_读写D3090","SINGLE","读写4WUB3091","读写","[4区]输出寄存器","16位 无符号二进制",3091]
[105,"设备0_读写D3580","SINGLE","读写4DUB3581","读写","[4区]输出寄存器","32位 无符号二进制",3581]
[106,"设备0_读写D3582","SINGLE","读写4DUB3583","读写","[4区]输出寄存器","32位 无符号二进制",3583]
[107,"设备0_读写D3584","SINGLE","读写4DUB3585","读写","[4区]输出寄存器","32位 无符号二进制",3585]
[108,"设备0_读写D3586","SINGLE","读写4DUB3587","读写","[4区]输出寄存器","32位 无符号二进制",3587]
[109,"设备0_读写D3680","SINGLE","读写4WUB3681","读写","[4区]输出寄存器","16位 无符号二进制",3681]
[110,"设备0_读写D3700","SINGLE","读写4WUB3701","读写","[4区]输出寄存器","16位 无符号二进制",3701]
[111,"设备0_读写D3702","SINGLE","读写4WUB3703","读写","[4区]输出寄存器","16位 无符号二进制",3703]
[112,"设备0_读写D3704","SINGLE","读写4WUB3705","读写","[4区]输出寄存器","16位 无符号二进制",3705]
[113,"设备0_读写D3706","SINGLE","读写4WUB3707","读写","[4区]输出寄存器","16位 无符号二进制",3707]
[114,"设备0_读写D3800","SINGLE","读写4WUB3801","读写","[4区]输出寄存器","16位 无符号二进制",3801]
[115,"设备0_读写D3802","SINGLE","读写4WUB3803","读写","[4区]输出寄存器","16位 无符号二进制",3803]
[116,"设备0_读写D3804","SINGLE","读写4WUB3805","读写","[4区]输出寄存器","16位 无符号二进制",3805]
[117,"设备0_读写D3806","SINGLE","读写4WUB3807","读写","[4区]输出寄存器","16位 无符号二进制",3807]
[118,"设备0_读写D4026","SINGLE","读写4DF4027","读写","[4区]输出寄存器","32位 浮点数",4027]
[119,"设备0_读写D4080","SINGLE","读写4DF4081","读写","[4区]输出寄存器","32位 浮点数",4081]
[120,"设备0_读写D4084","SINGLE","读写4DF4085","读写","[4区]输出寄存器","32位 浮点数",4085]
[121,"设备0_读写D4090","SINGLE","读写4WUB4091","读写","[4区]输出寄存器","16位 无符号二进制",4091]
[122,"设备0_读写D5026","SINGLE","读写4DF5027","读写","[4区]输出寄存器","32位 浮点数",5027]
[123,"设备0_读写D5080","SINGLE","读写4DF5081","读写","[4区]输出寄存器","32位 浮点数",5081]
[124,"设备0_读写D5084","SINGLE","读写4DF5085","读写","[4区]输出寄存器","32位 浮点数",5085]
[125,"设备0_读写D5090","SINGLE","读写4WUB5091","读写","[4区]输出寄存器","16位 无符号二进制",5091]
[126,"设备0_读写D6012","SINGLE","读写4DF6013","读写","[4区]输出寄存器","32位 浮点数",6013]
[127,"设备0_读写D6026","SINGLE","读写4DF6027","读写","[4区]输出寄存器","32位 浮点数",6027]
[128,"设备0_读写D6080","SINGLE","读写4DF6081","读写","[4区]输出寄存器","32位 浮点数",6081]
[129,"设备0_读写D6084","SINGLE","读写4DF6085","读写","[4区]输出寄存器","32位 浮点数",6085]
[130,"设备0_读写D6090","SINGLE","读写4WUB6091","读写","[4区]输出寄存器","16位 无符号二进制",6091]
[131,"设备0_读写D6300","SINGLE","读写4DF6301","读写","[4区]输出寄存器","32位 浮点数",6301]
[132,"设备0_读写D6304","SINGLE","读写4DF6305","读写","[4区]输出寄存器","32位 浮点数",6305]
[133,"设备0_读写D6308","SINGLE","读写4DF6309","读写","[4区]输出寄存器","32位 浮点数",6309]
[134,"设备0_读写D6312","SINGLE","读写4DF6313","读写","[4区]输出寄存器","32位 浮点数",6313]
[135,"设备0_读写D6316","SINGLE","读写4DF6317","读写","[4区]输出寄存器","32位 浮点数",6317]
[136,"设备0_读写D6320","SINGLE","读写4DF6321","读写","[4区]输出寄存器","32位 浮点数",6321]
[137,"设备0_读写D6322","SINGLE","读写4DF6323","读写","[4区]输出寄存器","32位 浮点数",6323]
[138,"设备0_读写D6324","SINGLE","读写4DF6325","读写","[4区]输出寄存器","32位 浮点数",6325]
[139,"设备0_读写D6326","SINGLE","读写4DF6327","读写","[4区]输出寄存器","32位 浮点数",6327]
[140,"设备0_读写D6328","SINGLE","读写4DF6329","读写","[4区]输出寄存器","32位 浮点数",6329]
[141,"设备0_读写D6330","SINGLE","读写4DF6331","读写","[4区]输出寄存器","32位 浮点数",6331]
[142,"设备0_读写D6332","SINGLE","读写4DF6333","读写","[4区]输出寄存器","32位 浮点数",6333]
[143,"设备0_读写D6334","SINGLE","读写4DF6335","读写","[4区]输出寄存器","32位 浮点数",6335]
[144,"设备0_读写D6336","SINGLE","读写4DF6337","读写","[4区]输出寄存器","32位 浮点数",6337]

{"sheet":"设备1","index":4,"n_rows":177,"n_cols":8,"rows_kept":177,"cut":false,"hidden":false,"merged":[]}
["通道号","变量名","变量类型","通道名称","读写类型","寄存器名称","数据类型","寄存器地址"]
[1,"设备1_只读X0002","INTEGER","只读163491","只读","[1区]输入继电器","NULL",63491]
[2,"设备1_只读X0003","INTEGER","只读163492","只读","[1区]输入继电器","NULL",63492]
[3,"设备1_只读X0004","INTEGER","只读163493","只读","[1区]输入继电器","NULL",63493]
[4,"设备1_读写M0000","INTEGER","读写00001","读写","[0区]输出继电器","NULL",1]
[5,"设备1_读写M0001","INTEGER","读写00002","读写","[0区]输出继电器","NULL",2]
[6,"设备1_读写M0002","INTEGER","读写00003","读写","[0区]输出继电器","NULL",3]
[7,"设备1_读写M0003","INTEGER","读写00004","读写","[0区]输出继电器","NULL",4]
[8,"设备1_读写M0020","INTEGER","读写00021","读写","[0区]输出继电器","NULL",21]
[9,"设备1_读写M0035","INTEGER","读写00036","读写","[0区]输出继电器","NULL",36]
[10,"设备1_读写M0150","INTEGER","读写00151","读写","[0区]输出继电器","NULL",151]
[11,"设备1_读写M0156","INTEGER","读写00157","读写","[0区]输出继电器","NULL",157]
[12,"设备1_读写M0350","INTEGER","读写00351","读写","[0区]输出继电器","NULL",351]
[13,"设备1_读写M0490","INTEGER","读写00491","读写","[0区]输出继电器","NULL",491]
[14,"设备1_读写M0500","INTEGER","读写00501","读写","[0区]输出继电器","NULL",501]
[15,"设备1_读写M0501","INTEGER","读写00502","读写","[0区]输出继电器","NULL",502]
[16,"设备1_读写M0502","INTEGER","读写00503","读写","[0区]输出继电器","NULL",503]
[17,"设备1_读写M0503","INTEGER","读写00504","读写","[0区]输出继电器","NULL",504]
[18,"设备1_读写M0510","INTEGER","读写00511","读写","[0区]输出继电器","NULL",511]
[19,"设备1_读写M0511","INTEGER","读写00512","读写","[0区]输出继电器","NULL",512]
[20,"设备1_读写M0512","INTEGER","读写00513","读写","[0区]输出继电器","NULL",513]
[21,"设备1_读写M0513","INTEGER","读写00514","读写","[0区]输出继电器","NULL",514]
[22,"设备1_读写M0540","INTEGER","读写00541","读写","[0区]输出继电器","NULL",541]
[23,"设备1_读写M0681","INTEGER","读写00682","读写","[0区]输出继电器","NULL",682]
[24,"设备1_读写M0684","INTEGER","读写00685","读写","[0区]输出继电器","NULL",685]
[25,"设备1_读写M0910","INTEGER","读写00911","读写","[0区]输出继电器","NULL",911]
[26,"设备1_读写M0920","INTEGER","读写00921","读写","[0区]输出继电器","NULL",921]
[27,"设备1_读写M927","INTEGER","读写00927","读写","[0区]输出继电器","NULL",927]
[28,"设备1_读写M0950","INTEGER","读写00951","读写","[0区]输出继电器","NULL",951]
[29,"设备1_读写M0951","INTEGER","读写00952","读写","[0区]输出继电器","NULL",952]
[30,"设备1_读写M0952","INTEGER","读写00953","读写","[0区]输出继电器","NULL",953]
[31,"设备1_读写M0953","INTEGER","读写00954","读写","[0区]输出继电器","NULL",954]
[32,"设备1_读写M0954","INTEGER","读写00955","读写","[0区]输出继电器","NULL",955]
[33,"设备1_读写M0955","INTEGER","读写00956","读写","[0区]输出继电器","NULL",956]
[34,"设备1_读写M0956","INTEGER","读写00957","读写","[0区]输出继电器","NULL",957]
[35,"设备1_读写M0957","INTEGER","读写00958","读写","[0区]输出继电器","NULL",958]
[36,"设备1_读写M0958","INTEGER","读写00959","读写","[0区]输出继电器","NULL",959]
[37,"设备1_读写M0959","INTEGER","读写00960","读写","[0区]输出继电器","NULL",960]
[38,"设备1_读写M0960","INTEGER","读写00961","读写","[0区]输出继电器","NULL",961]
[39,"设备1_读写M0961","INTEGER","读写00962","读写","[0区]输出继电器","NULL",962]
[40,"设备1_读写M0963","INTEGER","读写00964","读写","[0区]输出继电器","NULL",964]
[41,"设备1_读写M0964","INTEGER","读写00965","读写","[0区]输出继电器","NULL",965]
[42,"设备1_读写M0965","INTEGER","读写00966","读写","[0区]输出继电器","NULL",966]
[43,"设备1_读写M0966","INTEGER","读写00967","读写","[0区]输出继电器","NULL",967]
[44,"设备1_读写M0967","INTEGER","读写00968","读写","[0区]输出继电器","NULL",968]
[45,"设备1_读写M0968","INTEGER","读写00969","读写","[0区]输出继电器","NULL",969]
[46,"设备1_读写M0970","INTEGER","读写00971","读写","[0区]输出继电器","NULL",971]
[47,"设备1_读写M0971","INTEGER","读写00972","读写","[0区]输出继电器","NULL",972]
[48,"设备1_读写M1300","INTEGER","读写01301","读写","[0区]输出继电器","NULL",1301]
[49,"设备1_读写M3000","INTEGER","读写03001","读写","[0区]输出继电器","NULL",3001]
[50,"设备1_读写Y0001","INTEGER","读写064514","读写","[0区]输出继电器","NULL",64514]
[51,"设备1_读写Y0002","INTEGER","读写064515","读写","[0区]输出继电器","NULL",64515]
[52,"设备1_读写Y0003","INTEGER","读写064516","读写","[0区]输出继电器","NULL",64516]
[53,"设备1_读写Y0004","INTEGER","读写064517","读写","[0区]输出继电器","NULL",64517]
[54,"设备1_读写Y0005","INTEGER","读写064518","读写","[0区]输出继电器","NULL",64518]
[55,"设备1_读写D160","SINGLE","读写4DB0161","读写","[4区]输出寄存器","32位 有符号二进制",161]
[56,"设备1_读写D184","SINGLE","读写4DF0185","读写","[4区]输出寄存器","32位 浮点数",185]
[57,"设备1_读写D600","SINGLE","读写4DF0601","读写","[4区]输出寄存器","32位 浮点数",601]
[58,"设备1_读写D1000","SINGLE","读写4WUB1001","读写","[4区]输出寄存器","16位 无符号二进制",1001]
[59,"设备1_读写D1001","SINGLE","读写4WUB1002","读写","[4区]输出寄存器","16位 无符号二进制",1002]
[60,"设备1_读写D1002","SINGLE","读写4WUB1003","读写","[4区]输出寄存器","16位 无符号二进制",1003]
[61,"设备1_读写D1003","SINGLE","读写4WUB1004","读写","[4区]输出寄存器","16位 无符号二进制",1004]
[62,"设备1_读写D1184","SINGLE","读写4WUB1185","读写","[4区]输出寄存器","16位 无符号二进制",1185]
[63,"设备1_读写D2000","SINGLE","读写4WUB2001","读写","[4区]输出寄存器","16位 无符号二进制",2001]
[64,"设备1_读写D2002","SINGLE","读写4WUB2003","读写","[4区]输出寄存器","16位 无符号二进制",2003]
[65,"设备1_读写D2003","SINGLE","读写4WUB2004","读写","[4区]输出寄存器","16位 无符号二进制",2004]
[66,"设备1_读写D2004","SINGLE","读写4WUB2005","读写","[4区]输出寄存器","16位 无符号二进制",2005]
[67,"设备1_读写D2022","SINGLE","读写4WB2023","读写","[4区]输出寄存器","16位 有符号二进制",2023]
[68,"设备1_读写D2023","SINGLE","读写4WB2024","读写","[4区]输出寄存器","16位 有符号二进制",2024]
[69,"设备1_读写D2030","SINGLE","读写4WB2031","读写","[4区]输出寄存器","16位 有符号二进制",2031]
[70,"设备1_读写D2034","SINGLE","读写4WUB2035","读写","[4区]输出寄存器","16位 无符号二进制",2035]
[71,"设备1_读写D2040","SINGLE","读写4WUB2041","读写","[4区]输出寄存器","16位 无符号二进制",2041]
[72,"设备1_读写D2050","SINGLE","读写4WUB2051","读写","[4区]输出寄存器","16位 无符号二进制",2051]
[73,"设备1_读写D2058","SINGLE","读写4WB2059","读写","[4区]输出寄存器","16位 有符号二进制",2059]
[74,"设备1_读写D2132","SINGLE","读写4WUB2133","读写","[4区]输出寄存器","16位 无符号二进制",2133]
[75,"设备1_读写D2140","SINGLE","读写4WUB2141","读写","[4区]输出寄存器","16位 无符号二进制",2141]
[76,"设备1_读写D2144","SINGLE","读写4WUB2145","读写","[4区]输出寄存器","16位 无符号二进制",2145]
[77,"设备1_读写D2170","SINGLE","读写4WUB2171","读写","[4区]输出寄存器","16位 无符号二进制",2171]
[78,"设备1_读写D2182","SINGLE","读写4WUB2183","读写","[4区]输出寄存器","16位 无符号二进制",2183]
[79,"设备1_读写D2184","SINGLE","读写4WUB2185","读写","[4区]输出寄存器","16位 无符号二进制",2185]
[80,"设备1_读写D2308","SINGLE","读写4WUB2309","读写","[4区]输出寄存器","16位 无符号二进制",2309]
[81,"设备1_读写D2320","SINGLE","读写4WUB2321","读写","[4区]输出寄存器","16位 无符号二进制",2321]
[82,"设备1_读写D2324","SINGLE","读写4WUB2325","读写","[4区]输出寄存器","16位 无符号二进制",2325]
[83,"设备1_读写D2374","SINGLE","读写4WUB2375","读写","[4区]输出寄存器","16位 无符号二进制",2375]
[84,"设备1_读写D2398","SINGLE","读写4WUB2399","读写","[4区]输出寄存器","16位 无符号二进制",2399]
[85,"设备1_读写D2500","SINGLE","读写4WUB2501","读写","[4区]输出寄存器","16位 无符号二进制",2501]
[86,"设备1_读写D2501","SINGLE","读写4WUB2502","读写","[4区]输出寄存器","16位 无符号二进制",2502]
[87,"设备1_读写D2502","SINGLE","读写4WUB2503","读写","[4区]输出寄存器","16位 无符号二进制",2503]
[88,"设备1_读写D2503","SINGLE","读写4WUB2504","读写","[4区]输出寄存器","16位 无符号二进制",2504]
[89,"设备1_读写D2504","SINGLE","读写4WUB2505","读写","[4区]输出寄存器","16位 无符号二进制",2505]
[90,"设备1_读写D2505","SINGLE","读写4WUB2506","读写","[4区]输出寄存器","16位 无符号二进制",2506]
[91,"设备1_读写D2506","SINGLE","读写4WUB2507","读写","[4区]输出寄存器","16位 无符号二进制",2507]
[92,"设备1_读写D2507","SINGLE","读写4WUB2508","读写","[4区]输出寄存器","16位 无符号二进制",2508]
[93,"设备1_读写D2510","SINGLE","读写4DF2511","读写","[4区]输出寄存器","32位 浮点数",2511]
[94,"设备1_读写D2512","SINGLE","读写4DF2513","读写","[4区]输出寄存器","32位 浮点数",2513]
[95,"设备1_读写D2514","SINGLE","读写4DF2515","读写","[4区]输出寄存器","32位 浮点数",2515]
[96,"设备1_读写D2516","SINGLE","读写4DF2517","读写","[4区]输出寄存器","32位 浮点数",2517]
[97,"设备1_读写D2520","SINGLE","读写4WUB2521","读写","[4区]输出寄存器","16位 无符号二进制",2521]
[98,"设备1_读写D2521","SINGLE","读写4WUB2522","读写","[4区]输出寄存器","16位 无符号二进制",2522]
[99,"设备1_读写D2610","SINGLE","读写4WUB2611","读写","[4区]输出寄存器","16位 无符号二进制",2611]
[100,"设备1_读写D2620","SINGLE","读写4WUB2621","读写","[4区]输出寄存器","16位 无符号二进制",2621]
[101,"设备1_读写D2662","SINGLE","读写4WUB2663","读写","[4区]输出寄存器","16位 无符号二进制",2663]
[102,"设备1_读写D2700","SINGLE","读写4WUB2701","读写","[4区]输出寄存器","16位 无符号二进制",2701]
[103,"设备1_读写D2762","SINGLE","读写4WUB2763","读写","[4区]输出寄存器","16位 无符号二进制",2763]
[104,"设备1_读写D3026","SINGLE","读写4DF3027","读写","[4区]输出寄存器","32位 浮点数",3027]
[105,"设备1_读写D3080","SINGLE","读写4DF3081","读写","[4区]输出寄存器","32位 浮点数",3081]
[106,"设备1_读写D3084","SINGLE","读写4DF3085","读写","[4区]输出寄存器","32位 浮点数",3085]
[107,"设备1_读写D3090","SINGLE","读写4WUB3091","读写","[4区]输出寄存器","16位 无符号二进制",3091]
[108,"设备1_读写D3580","SINGLE","读写4DUB3581","读写","[4区]输出寄存器","32位 无符号二进制",3581]
[109,"设备1_读写D3582","SINGLE","读写4DUB3583","读写","[4区]输出寄存器","32位 无符号二进制",3583]
[110,"设备1_读写D3584","SINGLE","读写4DUB3585","读写","[4区]输出寄存器","32位 无符号二进制",3585]
[111,"设备1_读写D3586","SINGLE","读写4DUB3587","读写","[4区]输出寄存器","32位 无符号二进制",3587]
[112,"设备1_读写D3680","SINGLE","读写4WUB3681","读写","[4区]输出寄存器","16位 无符号二进制",3681]
[113,"设备1_读写D3700","SINGLE","读写4WUB3701","读写","[4区]输出寄存器","16位 无符号二进制",3701]
[114,"设备1_读写D3702","SINGLE","读写4WUB3703","读写","[4区]输出寄存器","16位 无符号二进制",3703]
[115,"设备1_读写D3704","SINGLE","读写4WUB3705","读写","[4区]输出寄存器","16位 无符号二进制",3705]
[116,"设备1_读写D3706","SINGLE","读写4WUB3707","读写","[4区]输出寄存器","16位 无符号二进制",3707]
[117,"设备1_读写D3710","SINGLE","读写4WUB3711","读写","[4区]输出寄存器","16位 无符号二进制",3711]
[118,"设备1_读写D3712","SINGLE","读写4WUB3713","读写","[4区]输出寄存器","16位 无符号二进制",3713]
[119,"设备1_读写D3800","SINGLE","读写4WUB3801","读写","[4区]输出寄存器","16位 无符号二进制",3801]
[120,"设备1_读写D3802","SINGLE","读写4WUB3803","读写","[4区]输出寄存器","16位 无符号二进制",3803]
[121,"设备1_读写D3804","SINGLE","读写4WUB3805","读写","[4区]输出寄存器","16位 无符号二进制",3805]
[122,"设备1_读写D3806","SINGLE","读写4WUB3807","读写","[4区]输出寄存器","16位 无符号二进制",3807]
[123,"设备1_读写4WUB3809","SINGLE","读写4WUB3809","读写","[4区]输出寄存器","16位 无符号二进制",3809]
[124,"设备1_读写4WUB3821","SINGLE","读写4WUB3821","读写","[4区]输出寄存器","16位 无符号二进制",3821]
[125,"设备1_读写D3830","SINGLE","读写4WUB3831","读写","[4区]输出寄存器","16位 无符号二进制",3831]
[126,"设备1_读写D3832","SINGLE","读写4WUB3833","读写","[4区]输出寄存器","16位 无符号二进制",3833]
[127,"设备1_读写D4026","SINGLE","读写4DF4027","读写","[4区]输出寄存器","32位 浮点数",4027]
[128,"设备1_读写D4080","SINGLE","读写4DF4081","读写","[4区]输出寄存器","32位 浮点数",4081]
[129,"设备1_读写D4084","SINGLE","读写4DF4085","读写","[4区]输出寄存器","32位 浮点数",4085]
[130,"设备1_读写D4090","SINGLE","读写4WUB4091","读写","[4区]输出寄存器","16位 无符号二进制",4091]
[131,"设备1_读写D5026","SINGLE","读写4DF5027","读写","[4区]输出寄存器","32位 浮点数",5027]
[132,"设备1_读写D5080","SINGLE","读写4DF5081","读写","[4区]输出寄存器","32位 浮点数",5081]
[133,"设备1_读写D5084","SINGLE","读写4DF5085","读写","[4区]输出寄存器","32位 浮点数",5085]
[134,"设备1_读写D5090","SINGLE","读写4WUB5091","读写","[4区]输出寄存器","16位 无符号二进制",5091]
[135,"设备1_读写D5850","SINGLE","读写4WUB5851","读写","[4区]输出寄存器","16位 无符号二进制",5851]
[136,"设备1_读写D6012","SINGLE","读写4DF6013","读写","[4区]输出寄存器","32位 浮点数",6013]
[137,"设备1_读写D6026","SINGLE","读写4DF6027","读写","[4区]输出寄存器","32位 浮点数",6027]
[138,"设备1_读写D6080","SINGLE","读写4DF6081","读写","[4区]输出寄存器","32位 浮点数",6081]
[139,"设备1_读写D6084","SINGLE","读写4DF6085","读写","[4区]输出寄存器","32位 浮点数",6085]
[140,"设备1_读写D6090","SINGLE","读写4WUB6091","读写","[4区]输出寄存器","16位 无符号二进制",6091]
[141,"设备1_读写D6300","SINGLE","读写4DF6301","读写","[4区]输出寄存器","32位 浮点数",6301]
[142,"设备1_读写D6304","SINGLE","读写4DF6305","读写","[4区]输出寄存器","32位 浮点数",6305]
[143,"设备1_读写D6308","SINGLE","读写4DF6309","读写","[4区]输出寄存器","32位 浮点数",6309]
[144,"设备1_读写D6312","SINGLE","读写4DF6313","读写","[4区]输出寄存器","32位 浮点数",6313]
[145,"设备1_读写D6316","SINGLE","读写4DF6317","读写","[4区]输出寄存器","32位 浮点数",6317]
[146,"设备1_读写D6320","SINGLE","读写4DF6321","读写","[4区]输出寄存器","32位 浮点数",6321]
[147,"设备1_读写D6322","SINGLE","读写4DF6323","读写","[4区]输出寄存器","32位 浮点数",6323]
[148,"设备1_读写D6324","SINGLE","读写4DF6325","读写","[4区]输出寄存器","32位 浮点数",6325]
[149,"设备1_读写D6326","SINGLE","读写4DF6327","读写","[4区]输出寄存器","32位 浮点数",6327]
[150,"设备1_读写D6328","SINGLE","读写4DF6329","读写","[4区]输出寄存器","32位 浮点数",6329]
[151,"设备1_读写D6330","SINGLE","读写4DF6331","读写","[4区]输出寄存器","32位 浮点数",6331]
[152,"设备1_读写D6332","SINGLE","读写4DF6333","读写","[4区]输出寄存器","32位 浮点数",6333]
[153,"设备1_读写D6334","SINGLE","读写4DF6335","读写","[4区]输出寄存器","32位 浮点数",6335]
[154,"设备1_读写D6336","SINGLE","读写4DF6337","读写","[4区]输出寄存器","32位 浮点数",6337]
[155,"设备1_读写D6850","SINGLE","读写4WUB6851","读写","[4区]输出寄存器","16位 无符号二进制",6851]
[156,"设备1_读写R1014","SINGLE","读写4DF13303","读写","[4区]输出寄存器","32位 浮点数",13303]
[157,"设备1_读写R1016","SINGLE","读写4DF13305","读写","[4区]输出寄存器","32位 浮点数",13305]
[158,"设备1_读写R1030","SINGLE","读写4DF13319","读写","[4区]输出寄存器","32位 浮点数",13319]
[159,"设备1_读写R1032","SINGLE","读写4DF13321","读写","[4区]输出寄存器","32位 浮点数",13321]
[160,"设备1_读写R1040","SINGLE","读写4DF13329","读写","[4区]输出寄存器","32位 浮点数",13329]
[161,"设备1_读写R1050","SINGLE","读写4DF13339","读写","[4区]输出寄存器","32位 浮点数",13339]
[162,"设备1_读写R1106","SINGLE","读写4DF13395","读写","[4区]输出寄存器","32位 浮点数",13395]
[163,"设备1_读写R1126","SINGLE","读写4DF13415","读写","[4区]输出寄存器","32位 浮点数",13415]
[164,"设备1_读写R1204","SINGLE","读写4DF13493","读写","[4区]输出寄存器","32位 浮点数",13493]
[165,"设备1_读写R1206","SINGLE","读写4DF13495","读写","[4区]输出寄存器","32位 浮点数",13495]
[166,"设备1_读写R1226","SINGLE","读写4DF13515","读写","[4区]输出寄存器","32位 浮点数",13515]
[167,"设备1_读写R1236","SINGLE","读写4DF13525","读写","[4区]输出寄存器","32位 浮点数",13525]
[168,"设备1_读写R1308","SINGLE","读写4DF13597","读写","[4区]输出寄存器","32位 浮点数",13597]
[169,"设备1_读写R1320","SINGLE","读写4DF13609","读写","[4区]输出寄存器","32位 浮点数",13609]
[170,"设备1_读写R1322","SINGLE","读写4DF13611","读写","[4区]输出寄存器","32位 浮点数",13611]
[171,"设备1_读写R1352","SINGLE","读写4DF13641","读写","[4区]输出寄存器","32位 浮点数",13641]
[172,"设备1_读写R1354","SINGLE","读写4DF13643","读写","[4区]输出寄存器","32位 浮点数",13643]
[173,"设备1_读写R1366","SINGLE","读写4DF13655","读写","[4区]输出寄存器","32位 浮点数",13655]
[174,"设备1_读写R1600","SINGLE","读写4DF13889","读写","[4区]输出寄存器","32位 浮点数",13889]
[175,"设备1_读写R1602","SINGLE","读写4DF13891","读写","[4区]输出寄存器","32位 浮点数",13891]
[176,"设备1_读写R1700","SINGLE","读写4DF13989","读写","[4区]输出寄存器","32位 浮点数",13989]

{"sheet":"设备2","index":5,"n_rows":145,"n_cols":8,"rows_kept":145,"cut":false,"hidden":false,"merged":[]}
["通道号","变量名","变量类型","通道名称","读写类型","寄存器名称","数据类型","寄存器地址"]
[1,"设备2_只读X0002","INTEGER","只读163491","只读","[1区]输入继电器","NULL",63491]
[2,"设备2_只读X0003","INTEGER","只读163492","只读","[1区]输入继电器","NULL",63492]
[3,"设备2_只读X0004","INTEGER","只读163493","只读","[1区]输入继电器","NULL",63493]
[4,"设备2_读写M0000","INTEGER","读写00001","读写","[0区]输出继电器","NULL",1]
[5,"设备2_读写M0020","INTEGER","读写00021","读写","[0区]输出继电器","NULL",21]
[6,"设备2_读写M0035","INTEGER","读写00036","读写","[0区]输出继电器","NULL",36]
[7,"设备2_读写M0150","INTEGER","读写00151","读写","[0区]输出继电器","NULL",151]
[8,"设备2_读写M0156","INTEGER","读写00157","读写","[0区]输出继电器","NULL",157]
[9,"设备2_读写M0350","INTEGER","读写00351","读写","[0区]输出继电器","NULL",351]
[10,"设备2_读写M0490","INTEGER","读写00491","读写","[0区]输出继电器","NULL",491]
[11,"设备2_读写M0500","INTEGER","读写00501","读写","[0区]输出继电器","NULL",501]
[12,"设备2_读写M0501","INTEGER","读写00502","读写","[0区]输出继电器","NULL",502]
[13,"设备2_读写M0502","INTEGER","读写00503","读写","[0区]输出继电器","NULL",503]
[14,"设备2_读写M0503","INTEGER","读写00504","读写","[0区]输出继电器","NULL",504]
[15,"设备2_读写M0510","INTEGER","读写00511","读写","[0区]输出继电器","NULL",511]
[16,"设备2_读写M0511","INTEGER","读写00512","读写","[0区]输出继电器","NULL",512]
[17,"设备2_读写M0512","INTEGER","读写00513","读写","[0区]输出继电器","NULL",513]
[18,"设备2_读写M0513","INTEGER","读写00514","读写","[0区]输出继电器","NULL",514]
[19,"设备2_读写M0540","INTEGER","读写00541","读写","[0区]输出继电器","NULL",541]
[20,"设备2_读写M0681","INTEGER","读写00682","读写","[0区]输出继电器","NULL",682]
[21,"设备2_读写M0684","INTEGER","读写00685","读写","[0区]输出继电器","NULL",685]
[22,"设备2_读写M0910","INTEGER","读写00911","读写","[0区]输出继电器","NULL",911]
[23,"设备2_读写M0920","INTEGER","读写00921","读写","[0区]输出继电器","NULL",921]
[24,"设备2_读写M927","INTEGER","读写00927","读写","[0区]输出继电器","NULL",927]
[25,"设备2_读写M0950","INTEGER","读写00951","读写","[0区]输出继电器","NULL",951]
[26,"设备2_读写M0951","INTEGER","读写00952","读写","[0区]输出继电器","NULL",952]
[27,"设备2_读写M0952","INTEGER","读写00953","读写","[0区]输出继电器","NULL",953]
[28,"设备2_读写M0953","INTEGER","读写00954","读写","[0区]输出继电器","NULL",954]
[29,"设备2_读写M0954","INTEGER","读写00955","读写","[0区]输出继电器","NULL",955]
[30,"设备2_读写M0955","INTEGER","读写00956","读写","[0区]输出继电器","NULL",956]
[31,"设备2_读写M0956","INTEGER","读写00957","读写","[0区]输出继电器","NULL",957]
[32,"设备2_读写M0957","INTEGER","读写00958","读写","[0区]输出继电器","NULL",958]
[33,"设备2_读写M0958","INTEGER","读写00959","读写","[0区]输出继电器","NULL",959]
[34,"设备2_读写M0959","INTEGER","读写00960","读写","[0区]输出继电器","NULL",960]
[35,"设备2_读写M0960","INTEGER","读写00961","读写","[0区]输出继电器","NULL",961]
[36,"设备2_读写M0961","INTEGER","读写00962","读写","[0区]输出继电器","NULL",962]
[37,"设备2_读写M0963","INTEGER","读写00964","读写","[0区]输出继电器","NULL",964]
[38,"设备2_读写M0964","INTEGER","读写00965","读写","[0区]输出继电器","NULL",965]
[39,"设备2_读写M0965","INTEGER","读写00966","读写","[0区]输出继电器","NULL",966]
[40,"设备2_读写M0966","INTEGER","读写00967","读写","[0区]输出继电器","NULL",967]
[41,"设备2_读写M0967","INTEGER","读写00968","读写","[0区]输出继电器","NULL",968]
[42,"设备2_读写M0968","INTEGER","读写00969","读写","[0区]输出继电器","NULL",969]
[43,"设备2_读写M0970","INTEGER","读写00971","读写","[0区]输出继电器","NULL",971]
[44,"设备2_读写M0971","INTEGER","读写00972","读写","[0区]输出继电器","NULL",972]
[45,"设备2_读写M1300","INTEGER","读写01301","读写","[0区]输出继电器","NULL",1301]
[46,"设备2_读写M3000","INTEGER","读写03001","读写","[0区]输出继电器","NULL",3001]
[47,"设备2_读写Y0001","INTEGER","读写064514","读写","[0区]输出继电器","NULL",64514]
[48,"设备2_读写Y0002","INTEGER","读写064515","读写","[0区]输出继电器","NULL",64515]
[49,"设备2_读写Y0003","INTEGER","读写064516","读写","[0区]输出继电器","NULL",64516]
[50,"设备2_读写Y0004","INTEGER","读写064517","读写","[0区]输出继电器","NULL",64517]
[51,"设备2_读写Y0005","INTEGER","读写064518","读写","[0区]输出继电器","NULL",64518]
[52,"设备2_读写D160","SINGLE","读写4DB0161","读写","[4区]输出寄存器","32位 有符号二进制",161]
[53,"设备2_读写D184","SINGLE","读写4DF0185","读写","[4区]输出寄存器","32位 浮点数",185]
[54,"设备2_读写D600","SINGLE","读写4DF0601","读写","[4区]输出寄存器","32位 浮点数",601]
[55,"设备2_读写D1000","SINGLE","读写4WUB1001","读写","[4区]输出寄存器","16位 无符号二进制",1001]
[56,"设备2_读写D1001","SINGLE","读写4WUB1002","读写","[4区]输出寄存器","16位 无符号二进制",1002]
[57,"设备2_读写D1002","SINGLE","读写4WUB1003","读写","[4区]输出寄存器","16位 无符号二进制",1003]
[58,"设备2_读写D1003","SINGLE","读写4WUB1004","读写","[4区]输出寄存器","16位 无符号二进制",1004]
[59,"设备2_读写D1184","SINGLE","读写4WUB1185","读写","[4区]输出寄存器","16位 无符号二进制",1185]
[60,"设备2_读写D2000","SINGLE","读写4WUB2001","读写","[4区]输出寄存器","16位 无符号二进制",2001]
[61,"设备2_读写D2002","SINGLE","读写4WUB2003","读写","[4区]输出寄存器","16位 无符号二进制",2003]
[62,"设备2_读写D2003","SINGLE","读写4WUB2004","读写","[4区]输出寄存器","16位 无符号二进制",2004]
[63,"设备2_读写D2004","SINGLE","读写4WUB2005","读写","[4区]输出寄存器","16位 无符号二进制",2005]
[64,"设备2_读写D2022","SINGLE","读写4WB2023","读写","[4区]输出寄存器","16位 有符号二进制",2023]
[65,"设备2_读写D2023","SINGLE","读写4WB2024","读写","[4区]输出寄存器","16位 有符号二进制",2024]
[66,"设备2_读写D2030","SINGLE","读写4WB2031","读写","[4区]输出寄存器","16位 有符号二进制",2031]
[67,"设备2_读写D2034","SINGLE","读写4WUB2035","读写","[4区]输出寄存器","16位 无符号二进制",2035]
[68,"设备2_读写D2040","SINGLE","读写4WUB2041","读写","[4区]输出寄存器","16位 无符号二进制",2041]
[69,"设备2_读写D2050","SINGLE","读写4WUB2051","读写","[4区]输出寄存器","16位 无符号二进制",2051]
[70,"设备2_读写D2058","SINGLE","读写4WB2059","读写","[4区]输出寄存器","16位 有符号二进制",2059]
[71,"设备2_读写D2132","SINGLE","读写4WUB2133","读写","[4区]输出寄存器","16位 无符号二进制",2133]
[72,"设备2_读写D2140","SINGLE","读写4WUB2141","读写","[4区]输出寄存器","16位 无符号二进制",2141]
[73,"设备2_读写D2144","SINGLE","读写4WUB2145","读写","[4区]输出寄存器","16位 无符号二进制",2145]
[74,"设备2_读写D2170","SINGLE","读写4WUB2171","读写","[4区]输出寄存器","16位 无符号二进制",2171]
[75,"设备2_读写D2182","SINGLE","读写4WUB2183","读写","[4区]输出寄存器","16位 无符号二进制",2183]
[76,"设备2_读写D2184","SINGLE","读写4WUB2185","读写","[4区]输出寄存器","16位 无符号二进制",2185]
[77,"设备2_读写D2308","SINGLE","读写4WUB2309","读写","[4区]输出寄存器","16位 无符号二进制",2309]
[78,"设备2_读写D2320","SINGLE","读写4WUB2321","读写","[4区]输出寄存器","16位 无符号二进制",2321]
[79,"设备2_读写D2324","SINGLE","读写4WUB2325","读写","[4区]输出寄存器","16位 无符号二进制",2325]
[80,"设备2_读写D2374","SINGLE","读写4WUB2375","读写","[4区]输出寄存器","16位 无符号二进制",2375]
[81,"设备2_读写D2398","SINGLE","读写4WUB2399","读写","[4区]输出寄存器","16位 无符号二进制",2399]
[82,"设备2_读写D2500","SINGLE","读写4WUB2501","读写","[4区]输出寄存器","16位 无符号二进制",2501]
[83,"设备2_读写D2501","SINGLE","读写4WUB2502","读写","[4区]输出寄存器","16位 无符号二进制",2502]
[84,"设备2_读写D2502","SINGLE","读写4WUB2503","读写","[4区]输出寄存器","16位 无符号二进制",2503]
[85,"设备2_读写D2503","SINGLE","读写4WUB2504","读写","[4区]输出寄存器","16位 无符号二进制",2504]
[86,"设备2_读写D2504","SINGLE","读写4WUB2505","读写","[4区]输出寄存器","16位 无符号二进制",2505]
[87,"设备2_读写D2505","SINGLE","读写4WUB2506","读写","[4区]输出寄存器","16位 无符号二进制",2506]
[88,"设备2_读写D2506","SINGLE","读写4WUB2507","读写","[4区]输出寄存器","16位 无符号二进制",2507]
[89,"设备2_读写D2507","SINGLE","读写4WUB2508","读写","[4区]输出寄存器","16位 无符号二进制",2508]
[90,"设备2_读写D2510","SINGLE","读写4DF2511","读写","[4区]输出寄存器","32位 浮点数",2511]
[91,"设备2_读写D2512","SINGLE","读写4DF2513","读写","[4区]输出寄存器","32位 浮点数",2513]
[92,"设备2_读写D2514","SINGLE","读写4DF2515","读写","[4区]输出寄存器","32位 浮点数",2515]
[93,"设备2_读写D2516","SINGLE","读写4DF2517","读写","[4区]输出寄存器","32位 浮点数",2517]
[94,"设备2_读写D2520","SINGLE","读写4WUB2521","读写","[4区]输出寄存器","16位 无符号二进制",2521]
[95,"设备2_读写D2521","SINGLE","读写4WUB2522","读写","[4区]输出寄存器","16位 无符号二进制",2522]
[96,"设备2_读写D2610","SINGLE","读写4WUB2611","读写","[4区]输出寄存器","16位 无符号二进制",2611]
[97,"设备2_读写D2620","SINGLE","读写4WUB2621","读写","[4区]输出寄存器","16位 无符号二进制",2621]
[98,"设备2_读写D2662","SINGLE","读写4WUB2663","读写","[4区]输出寄存器","16位 无符号二进制",2663]
[99,"设备2_读写D2700","SINGLE","读写4WUB2701","读写","[4区]输出寄存器","16位 无符号二进制",2701]
[100,"设备2_读写D2762","SINGLE","读写4WUB2763","读写","[4区]输出寄存器","16位 无符号二进制",2763]
[101,"设备2_读写D3026","SINGLE","读写4DF3027","读写","[4区]输出寄存器","32位 浮点数",3027]
[102,"设备2_读写D3080","SINGLE","读写4DF3081","读写","[4区]输出寄存器","32位 浮点数",3081]
[103,"设备2_读写D3084","SINGLE","读写4DF3085","读写","[4区]输出寄存器","32位 浮点数",3085]
[104,"设备2_读写D3090","SINGLE","读写4WUB3091","读写","[4区]输出寄存器","16位 无符号二进制",3091]
[105,"设备2_读写D3580","SINGLE","读写4DUB3581","读写","[4区]输出寄存器","32位 无符号二进制",3581]
[106,"设备2_读写D3582","SINGLE","读写4DUB3583","读写","[4区]输出寄存器","32位 无符号二进制",3583]
[107,"设备2_读写D3584","SINGLE","读写4DUB3585","读写","[4区]输出寄存器","32位 无符号二进制",3585]
[108,"设备2_读写D3586","SINGLE","读写4DUB3587","读写","[4区]输出寄存器","32位 无符号二进制",3587]
[109,"设备2_读写D3680","SINGLE","读写4WUB3681","读写","[4区]输出寄存器","16位 无符号二进制",3681]
[110,"设备2_读写D3700","SINGLE","读写4WUB3701","读写","[4区]输出寄存器","16位 无符号二进制",3701]
[111,"设备2_读写D3702","SINGLE","读写4WUB3703","读写","[4区]输出寄存器","16位 无符号二进制",3703]
[112,"设备2_读写D3704","SINGLE","读写4WUB3705","读写","[4区]输出寄存器","16位 无符号二进制",3705]
[113,"设备2_读写D3706","SINGLE","读写4WUB3707","读写","[4区]输出寄存器","16位 无符号二进制",3707]
[114,"设备2_读写D3800","SINGLE","读写4WUB3801","读写","[4区]输出寄存器","16位 无符号二进制",3801]
[115,"设备2_读写D3802","SINGLE","读写4WUB3803","读写","[4区]输出寄存器","16位 无符号二进制",3803]
[116,"设备2_读写D3804","SINGLE","读写4WUB3805","读写","[4区]输出寄存器","16位 无符号二进制",3805]
[117,"设备2_读写D3806","SINGLE","读写4WUB3807","读写","[4区]输出寄存器","16位 无符号二进制",3807]
[118,"设备2_读写D4026","SINGLE","读写4DF4027","读写","[4区]输出寄存器","32位 浮点数",4027]
[119,"设备2_读写D4080","SINGLE","读写4DF4081","读写","[4区]输出寄存器","32位 浮点数",4081]
[120,"设备2_读写D4084","SINGLE","读写4DF4085","读写","[4区]输出寄存器","32位 浮点数",4085]
[121,"设备2_读写D4090","SINGLE","读写4WUB4091","读写","[4区]输出寄存器","16位 无符号二进制",4091]
[122,"设备2_读写D5026","SINGLE","读写4DF5027","读写","[4区]输出寄存器","32位 浮点数",5027]
[123,"设备2_读写D5080","SINGLE","读写4DF5081","读写","[4区]输出寄存器","32位 浮点数",5081]
[124,"设备2_读写D5084","SINGLE","读写4DF5085","读写","[4区]输出寄存器","32位 浮点数",5085]
[125,"设备2_读写D5090","SINGLE","读写4WUB5091","读写","[4区]输出寄存器","16位 无符号二进制",5091]
[126,"设备2_读写D6012","SINGLE","读写4DF6013","读写","[4区]输出寄存器","32位 浮点数",6013]
[127,"设备2_读写D6026","SINGLE","读写4DF6027","读写","[4区]输出寄存器","32位 浮点数",6027]
[128,"设备2_读写D6080","SINGLE","读写4DF6081","读写","[4区]输出寄存器","32位 浮点数",6081]
[129,"设备2_读写D6084","SINGLE","读写4DF6085","读写","[4区]输出寄存器","32位 浮点数",6085]
[130,"设备2_读写D6090","SINGLE","读写4WUB6091","读写","[4区]输出寄存器","16位 无符号二进制",6091]
[131,"设备2_读写D6300","SINGLE","读写4DF6301","读写","[4区]输出寄存器","32位 浮点数",6301]
[132,"设备2_读写D6304","SINGLE","读写4DF6305","读写","[4区]输出寄存器","32位 浮点数",6305]
[133,"设备2_读写D6308","SINGLE","读写4DF6309","读写","[4区]输出寄存器","32位 浮点数",6309]
[134,"设备2_读写D6312","SINGLE","读写4DF6313","读写","[4区]输出寄存器","32位 浮点数",6313]
[135,"设备2_读写D6316","SINGLE","读写4DF6317","读写","[4区]输出寄存器","32位 浮点数",6317]
[136,"设备2_读写D6320","SINGLE","读写4DF6321","读写","[4区]输出寄存器","32位 浮点数",6321]
[137,"设备2_读写D6322","SINGLE","读写4DF6323","读写","[4区]输出寄存器","32位 浮点数",6323]
[138,"设备2_读写D6324","SINGLE","读写4DF6325","读写","[4区]输出寄存器","32位 浮点数",6325]
[139,"设备2_读写D6326","SINGLE","读写4DF6327","读写","[4区]输出寄存器","32位 浮点数",6327]
[140,"设备2_读写D6328","SINGLE","读写4DF6329","读写","[4区]输出寄存器","32位 浮点数",6329]
[141,"设备2_读写D6330","SINGLE","读写4DF6331","读写","[4区]输出寄存器","32位 浮点数",6331]
[142,"设备2_读写D6332","SINGLE","读写4DF6333","读写","[4区]输出寄存器","32位 浮点数",6333]
[143,"设备2_读写D6334","SINGLE","读写4DF6335","读写","[4区]输出寄存器","32位 浮点数",6335]
[144,"设备2_读写D6336","SINGLE","读写4DF6337","读写","[4区]输出寄存器","32位 浮点数",6337]

{"sheet":"设备3","index":6,"n_rows":145,"n_cols":8,"rows_kept":145,"cut":false,"hidden":false,"merged":[]}
["通道号","变量名","变量类型","通道名称","读写类型","寄存器名称","数据类型","寄存器地址"]
[1,"设备3_只读X0002","INTEGER","只读163491","只读","[1区]输入继电器","NULL",63491]
[2,"设备3_只读X0003","INTEGER","只读163492","只读","[1区]输入继电器","NULL",63492]
[3,"设备3_只读X0004","INTEGER","只读163493","只读","[1区]输入继电器","NULL",63493]
[4,"设备3_读写M0000","INTEGER","读写00001","读写","[0区]输出继电器","NULL",1]
[5,"设备3_读写M0020","INTEGER","读写00021","读写","[0区]输出继电器","NULL",21]
[6,"设备3_读写M0035","INTEGER","读写00036","读写","[0区]输出继电器","NULL",36]
[7,"设备3_读写M0150","INTEGER","读写00151","读写","[0区]输出继电器","NULL",151]
[8,"设备3_读写M0156","INTEGER","读写00157","读写","[0区]输出继电器","NULL",157]
[9,"设备3_读写M0350","INTEGER","读写00351","读写","[0区]输出继电器","NULL",351]
[10,"设备3_读写M0490","INTEGER","读写00491","读写","[0区]输出继电器","NULL",491]
[11,"设备3_读写M0500","INTEGER","读写00501","读写","[0区]输出继电器","NULL",501]
[12,"设备3_读写M0501","INTEGER","读写00502","读写","[0区]输出继电器","NULL",502]
[13,"设备3_读写M0502","INTEGER","读写00503","读写","[0区]输出继电器","NULL",503]
[14,"设备3_读写M0503","INTEGER","读写00504","读写","[0区]输出继电器","NULL",504]
[15,"设备3_读写M0510","INTEGER","读写00511","读写","[0区]输出继电器","NULL",511]
[16,"设备3_读写M0511","INTEGER","读写00512","读写","[0区]输出继电器","NULL",512]
[17,"设备3_读写M0512","INTEGER","读写00513","读写","[0区]输出继电器","NULL",513]
[18,"设备3_读写M0513","INTEGER","读写00514","读写","[0区]输出继电器","NULL",514]
[19,"设备3_读写M0540","INTEGER","读写00541","读写","[0区]输出继电器","NULL",541]
[20,"设备3_读写M0681","INTEGER","读写00682","读写","[0区]输出继电器","NULL",682]
[21,"设备3_读写M0684","INTEGER","读写00685","读写","[0区]输出继电器","NULL",685]
[22,"设备3_读写M0910","INTEGER","读写00911","读写","[0区]输出继电器","NULL",911]
[23,"设备3_读写M0920","INTEGER","读写00921","读写","[0区]输出继电器","NULL",921]
[24,"设备3_读写M927","INTEGER","读写00927","读写","[0区]输出继电器","NULL",927]
[25,"设备3_读写M0950","INTEGER","读写00951","读写","[0区]输出继电器","NULL",951]
[26,"设备3_读写M0951","INTEGER","读写00952","读写","[0区]输出继电器","NULL",952]
[27,"设备3_读写M0952","INTEGER","读写00953","读写","[0区]输出继电器","NULL",953]
[28,"设备3_读写M0953","INTEGER","读写00954","读写","[0区]输出继电器","NULL",954]
[29,"设备3_读写M0954","INTEGER","读写00955","读写","[0区]输出继电器","NULL",955]
[30,"设备3_读写M0955","INTEGER","读写00956","读写","[0区]输出继电器","NULL",956]
[31,"设备3_读写M0956","INTEGER","读写00957","读写","[0区]输出继电器","NULL",957]
[32,"设备3_读写M0957","INTEGER","读写00958","读写","[0区]输出继电器","NULL",958]
[33,"设备3_读写M0958","INTEGER","读写00959","读写","[0区]输出继电器","NULL",959]
[34,"设备3_读写M0959","INTEGER","读写00960","读写","[0区]输出继电器","NULL",960]
[35,"设备3_读写M0960","INTEGER","读写00961","读写","[0区]输出继电器","NULL",961]
[36,"设备3_读写M0961","INTEGER","读写00962","读写","[0区]输出继电器","NULL",962]
[37,"设备3_读写M0963","INTEGER","读写00964","读写","[0区]输出继电器","NULL",964]
[38,"设备3_读写M0964","INTEGER","读写00965","读写","[0区]输出继电器","NULL",965]
[39,"设备3_读写M0965","INTEGER","读写00966","读写","[0区]输出继电器","NULL",966]
[40,"设备3_读写M0966","INTEGER","读写00967","读写","[0区]输出继电器","NULL",967]
[41,"设备3_读写M0967","INTEGER","读写00968","读写","[0区]输出继电器","NULL",968]
[42,"设备3_读写M0968","INTEGER","读写00969","读写","[0区]输出继电器","NULL",969]
[43,"设备3_读写M0970","INTEGER","读写00971","读写","[0区]输出继电器","NULL",971]
[44,"设备3_读写M0971","INTEGER","读写00972","读写","[0区]输出继电器","NULL",972]
[45,"设备3_读写M1300","INTEGER","读写01301","读写","[0区]输出继电器","NULL",1301]
[46,"设备3_读写M3000","INTEGER","读写03001","读写","[0区]输出继电器","NULL",3001]
[47,"设备3_读写Y0001","INTEGER","读写064514","读写","[0区]输出继电器","NULL",64514]
[48,"设备3_读写Y0002","INTEGER","读写064515","读写","[0区]输出继电器","NULL",64515]
[49,"设备3_读写Y0003","INTEGER","读写064516","读写","[0区]输出继电器","NULL",64516]
[50,"设备3_读写Y0004","INTEGER","读写064517","读写","[0区]输出继电器","NULL",64517]
[51,"设备3_读写Y0005","INTEGER","读写064518","读写","[0区]输出继电器","NULL",64518]
[52,"设备3_读写D160","SINGLE","读写4DB0161","读写","[4区]输出寄存器","32位 有符号二进制",161]
[53,"设备3_读写D184","SINGLE","读写4DF0185","读写","[4区]输出寄存器","32位 浮点数",185]
[54,"设备3_读写D600","SINGLE","读写4DF0601","读写","[4区]输出寄存器","32位 浮点数",601]
[55,"设备3_读写D1000","SINGLE","读写4WUB1001","读写","[4区]输出寄存器","16位 无符号二进制",1001]
[56,"设备3_读写D1001","SINGLE","读写4WUB1002","读写","[4区]输出寄存器","16位 无符号二进制",1002]
[57,"设备3_读写D1002","SINGLE","读写4WUB1003","读写","[4区]输出寄存器","16位 无符号二进制",1003]
[58,"设备3_读写D1003","SINGLE","读写4WUB1004","读写","[4区]输出寄存器","16位 无符号二进制",1004]
[59,"设备3_读写D1184","SINGLE","读写4WUB1185","读写","[4区]输出寄存器","16位 无符号二进制",1185]
[60,"设备3_读写D2000","SINGLE","读写4WUB2001","读写","[4区]输出寄存器","16位 无符号二进制",2001]
[61,"设备3_读写D2002","SINGLE","读写4WUB2003","读写","[4区]输出寄存器","16位 无符号二进制",2003]
[62,"设备3_读写D2003","SINGLE","读写4WUB2004","读写","[4区]输出寄存器","16位 无符号二进制",2004]
[63,"设备3_读写D2004","SINGLE","读写4WUB2005","读写","[4区]输出寄存器","16位 无符号二进制",2005]
[64,"设备3_读写D2022","SINGLE","读写4WB2023","读写","[4区]输出寄存器","16位 有符号二进制",2023]
[65,"设备3_读写D2023","SINGLE","读写4WB2024","读写","[4区]输出寄存器","16位 有符号二进制",2024]
[66,"设备3_读写D2030","SINGLE","读写4WB2031","读写","[4区]输出寄存器","16位 有符号二进制",2031]
[67,"设备3_读写D2034","SINGLE","读写4WUB2035","读写","[4区]输出寄存器","16位 无符号二进制",2035]
[68,"设备3_读写D2040","SINGLE","读写4WUB2041","读写","[4区]输出寄存器","16位 无符号二进制",2041]
[69,"设备3_读写D2050","SINGLE","读写4WUB2051","读写","[4区]输出寄存器","16位 无符号二进制",2051]
[70,"设备3_读写D2058","SINGLE","读写4WB2059","读写","[4区]输出寄存器","16位 有符号二进制",2059]
[71,"设备3_读写D2132","SINGLE","读写4WUB2133","读写","[4区]输出寄存器","16位 无符号二进制",2133]
[72,"设备3_读写D2140","SINGLE","读写4WUB2141","读写","[4区]输出寄存器","16位 无符号二进制",2141]
[73,"设备3_读写D2144","SINGLE","读写4WUB2145","读写","[4区]输出寄存器","16位 无符号二进制",2145]
[74,"设备3_读写D2170","SINGLE","读写4WUB2171","读写","[4区]输出寄存器","16位 无符号二进制",2171]
[75,"设备3_读写D2182","SINGLE","读写4WUB2183","读写","[4区]输出寄存器","16位 无符号二进制",2183]
[76,"设备3_读写D2184","SINGLE","读写4WUB2185","读写","[4区]输出寄存器","16位 无符号二进制",2185]
[77,"设备3_读写D2308","SINGLE","读写4WUB2309","读写","[4区]输出寄存器","16位 无符号二进制",2309]
[78,"设备3_读写D2320","SINGLE","读写4WUB2321","读写","[4区]输出寄存器","16位 无符号二进制",2321]
[79,"设备3_读写D2324","SINGLE","读写4WUB2325","读写","[4区]输出寄存器","16位 无符号二进制",2325]
[80,"设备3_读写D2374","SINGLE","读写4WUB2375","读写","[4区]输出寄存器","16位 无符号二进制",2375]
[81,"设备3_读写D2398","SINGLE","读写4WUB2399","读写","[4区]输出寄存器","16位 无符号二进制",2399]
[82,"设备3_读写D2500","SINGLE","读写4WUB2501","读写","[4区]输出寄存器","16位 无符号二进制",2501]
[83,"设备3_读写D2501","SINGLE","读写4WUB2502","读写","[4区]输出寄存器","16位 无符号二进制",2502]
[84,"设备3_读写D2502","SINGLE","读写4WUB2503","读写","[4区]输出寄存器","16位 无符号二进制",2503]
[85,"设备3_读写D2503","SINGLE","读写4WUB2504","读写","[4区]输出寄存器","16位 无符号二进制",2504]
[86,"设备3_读写D2504","SINGLE","读写4WUB2505","读写","[4区]输出寄存器","16位 无符号二进制",2505]
[87,"设备3_读写D2505","SINGLE","读写4WUB2506","读写","[4区]输出寄存器","16位 无符号二进制",2506]
[88,"设备3_读写D2506","SINGLE","读写4WUB2507","读写","[4区]输出寄存器","16位 无符号二进制",2507]
[89,"设备3_读写D2507","SINGLE","读写4WUB2508","读写","[4区]输出寄存器","16位 无符号二进制",2508]
[90,"设备3_读写D2510","SINGLE","读写4DF2511","读写","[4区]输出寄存器","32位 浮点数",2511]
[91,"设备3_读写D2512","SINGLE","读写4DF2513","读写","[4区]输出寄存器","32位 浮点数",2513]
[92,"设备3_读写D2514","SINGLE","读写4DF2515","读写","[4区]输出寄存器","32位 浮点数",2515]
[93,"设备3_读写D2516","SINGLE","读写4DF2517","读写","[4区]输出寄存器","32位 浮点数",2517]
[94,"设备3_读写D2520","SINGLE","读写4WUB2521","读写","[4区]输出寄存器","16位 无符号二进制",2521]
[95,"设备3_读写D2521","SINGLE","读写4WUB2522","读写","[4区]输出寄存器","16位 无符号二进制",2522]
[96,"设备3_读写D2610","SINGLE","读写4WUB2611","读写","[4区]输出寄存器","16位 无符号二进制",2611]
[97,"设备3_读写D2620","SINGLE","读写4WUB2621","读写","[4区]输出寄存器","16位 无符号二进制",2621]
[98,"设备3_读写D2662","SINGLE","读写4WUB2663","读写","[4区]输出寄存器","16位 无符号二进制",2663]
[99,"设备3_读写D2700","SINGLE","读写4WUB2701","读写","[4区]输出寄存器","16位 无符号二进制",2701]
[100,"设备3_读写D2762","SINGLE","读写4WUB2763","读写","[4区]输出寄存器","16位 无符号二进制",2763]
[101,"设备3_读写D3026","SINGLE","读写4DF3027","读写","[4区]输出寄存器","32位 浮点数",3027]
[102,"设备3_读写D3080","SINGLE","读写4DF3081","读写","[4区]输出寄存器","32位 浮点数",3081]
[103,"设备3_读写D3084","SINGLE","读写4DF3085","读写","[4区]输出寄存器","32位 浮点数",3085]
[104,"设备3_读写D3090","SINGLE","读写4WUB3091","读写","[4区]输出寄存器","16位 无符号二进制",3091]
[105,"设备3_读写D3580","SINGLE","读写4DUB3581","读写","[4区]输出寄存器","32位 无符号二进制",3581]
[106,"设备3_读写D3582","SINGLE","读写4DUB3583","读写","[4区]输出寄存器","32位 无符号二进制",3583]
[107,"设备3_读写D3584","SINGLE","读写4DUB3585","读写","[4区]输出寄存器","32位 无符号二进制",3585]
[108,"设备3_读写D3586","SINGLE","读写4DUB3587","读写","[4区]输出寄存器","32位 无符号二进制",3587]
[109,"设备3_读写D3680","SINGLE","读写4WUB3681","读写","[4区]输出寄存器","16位 无符号二进制",3681]
[110,"设备3_读写D3700","SINGLE","读写4WUB3701","读写","[4区]输出寄存器","16位 无符号二进制",3701]
[111,"设备3_读写D3702","SINGLE","读写4WUB3703","读写","[4区]输出寄存器","16位 无符号二进制",3703]
[112,"设备3_读写D3704","SINGLE","读写4WUB3705","读写","[4区]输出寄存器","16位 无符号二进制",3705]
[113,"设备3_读写D3706","SINGLE","读写4WUB3707","读写","[4区]输出寄存器","16位 无符号二进制",3707]
[114,"设备3_读写D3800","SINGLE","读写4WUB3801","读写","[4区]输出寄存器","16位 无符号二进制",3801]
[115,"设备3_读写D3802","SINGLE","读写4WUB3803","读写","[4区]输出寄存器","16位 无符号二进制",3803]
[116,"设备3_读写D3804","SINGLE","读写4WUB3805","读写","[4区]输出寄存器","16位 无符号二进制",3805]
[117,"设备3_读写D3806","SINGLE","读写4WUB3807","读写","[4区]输出寄存器","16位 无符号二进制",3807]
[118,"设备3_读写D4026","SINGLE","读写4DF4027","读写","[4区]输出寄存器","32位 浮点数",4027]
[119,"设备3_读写D4080","SINGLE","读写4DF4081","读写","[4区]输出寄存器","32位 浮点数",4081]
[120,"设备3_读写D4084","SINGLE","读写4DF4085","读写","[4区]输出寄存器","32位 浮点数",4085]
[121,"设备3_读写D4090","SINGLE","读写4WUB4091","读写","[4区]输出寄存器","16位 无符号二进制",4091]
[122,"设备3_读写D5026","SINGLE","读写4DF5027","读写","[4区]输出寄存器","32位 浮点数",5027]
[123,"设备3_读写D5080","SINGLE","读写4DF5081","读写","[4区]输出寄存器","32位 浮点数",5081]
[124,"设备3_读写D5084","SINGLE","读写4DF5085","读写","[4区]输出寄存器","32位 浮点数",5085]
[125,"设备3_读写D5090","SINGLE","读写4WUB5091","读写","[4区]输出寄存器","16位 无符号二进制",5091]
[126,"设备3_读写D6012","SINGLE","读写4DF6013","读写","[4区]输出寄存器","32位 浮点数",6013]
[127,"设备3_读写D6026","SINGLE","读写4DF6027","读写","[4区]输出寄存器","32位 浮点数",6027]
[128,"设备3_读写D6080","SINGLE","读写4DF6081","读写","[4区]输出寄存器","32位 浮点数",6081]
[129,"设备3_读写D6084","SINGLE","读写4DF6085","读写","[4区]输出寄存器","32位 浮点数",6085]
[130,"设备3_读写D6090","SINGLE","读写4WUB6091","读写","[4区]输出寄存器","16位 无符号二进制",6091]
[131,"设备3_读写D6300","SINGLE","读写4DF6301","读写","[4区]输出寄存器","32位 浮点数",6301]
[132,"设备3_读写D6304","SINGLE","读写4DF6305","读写","[4区]输出寄存器","32位 浮点数",6305]
[133,"设备3_读写D6308","SINGLE","读写4DF6309","读写","[4区]输出寄存器","32位 浮点数",6309]
[134,"设备3_读写D6312","SINGLE","读写4DF6313","读写","[4区]输出寄存器","32位 浮点数",6313]
[135,"设备3_读写D6316","SINGLE","读写4DF6317","读写","[4区]输出寄存器","32位 浮点数",6317]
[136,"设备3_读写D6320","SINGLE","读写4DF6321","读写","[4区]输出寄存器","32位 浮点数",6321]
[137,"设备3_读写D6322","SINGLE","读写4DF6323","读写","[4区]输出寄存器","32位 浮点数",6323]
[138,"设备3_读写D6324","SINGLE","读写4DF6325","读写","[4区]输出寄存器","32位 浮点数",6325]
[139,"设备3_读写D6326","SINGLE","读写4DF6327","读写","[4区]输出寄存器","32位 浮点数",6327]
[140,"设备3_读写D6328","SINGLE","读写4DF6329","读写","[4区]输出寄存器","32位 浮点数",6329]
[141,"设备3_读写D6330","SINGLE","读写4DF6331","读写","[4区]输出寄存器","32位 浮点数",6331]
[142,"设备3_读写D6332","SINGLE","读写4DF6333","读写","[4区]输出寄存器","32位 浮点数",6333]
[143,"设备3_读写D6334","SINGLE","读写4DF6335","读写","[4区]输出寄存器","32位 浮点数",6335]
[144,"设备3_读写D6336","SINGLE","读写4DF6337","读写","[4区]输出寄存器","32位 浮点数",6337]

{"sheet":"设备4","index":7,"n_rows":145,"n_cols":8,"rows_kept":145,"cut":false,"hidden":false,"merged":[]}
["通道号","变量名","变量类型","通道名称","读写类型","寄存器名称","数据类型","寄存器地址"]
[1,"设备4_只读X0002","INTEGER","只读163491","只读","[1区]输入继电器","NULL",63491]
[2,"设备4_只读X0003","INTEGER","只读163492","只读","[1区]输入继电器","NULL",63492]
[3,"设备4_只读X0004","INTEGER","只读163493","只读","[1区]输入继电器","NULL",63493]
[4,"设备4_读写M0000","INTEGER","读写00001","读写","[0区]输出继电器","NULL",1]
[5,"设备4_读写M0020","INTEGER","读写00021","读写","[0区]输出继电器","NULL",21]
[6,"设备4_读写M0035","INTEGER","读写00036","读写","[0区]输出继电器","NULL",36]
[7,"设备4_读写M0150","INTEGER","读写00151","读写","[0区]输出继电器","NULL",151]
[8,"设备4_读写M0156","INTEGER","读写00157","读写","[0区]输出继电器","NULL",157]
[9,"设备4_读写M0350","INTEGER","读写00351","读写","[0区]输出继电器","NULL",351]
[10,"设备4_读写M0490","INTEGER","读写00491","读写","[0区]输出继电器","NULL",491]
[11,"设备4_读写M0500","INTEGER","读写00501","读写","[0区]输出继电器","NULL",501]
[12,"设备4_读写M0501","INTEGER","读写00502","读写","[0区]输出继电器","NULL",502]
[13,"设备4_读写M0502","INTEGER","读写00503","读写","[0区]输出继电器","NULL",503]
[14,"设备4_读写M0503","INTEGER","读写00504","读写","[0区]输出继电器","NULL",504]
[15,"设备4_读写M0510","INTEGER","读写00511","读写","[0区]输出继电器","NULL",511]
[16,"设备4_读写M0511","INTEGER","读写00512","读写","[0区]输出继电器","NULL",512]
[17,"设备4_读写M0512","INTEGER","读写00513","读写","[0区]输出继电器","NULL",513]
[18,"设备4_读写M0513","INTEGER","读写00514","读写","[0区]输出继电器","NULL",514]
[19,"设备4_读写M0540","INTEGER","读写00541","读写","[0区]输出继电器","NULL",541]
[20,"设备4_读写M0681","INTEGER","读写00682","读写","[0区]输出继电器","NULL",682]
[21,"设备4_读写M0684","INTEGER","读写00685","读写","[0区]输出继电器","NULL",685]
[22,"设备4_读写M0910","INTEGER","读写00911","读写","[0区]输出继电器","NULL",911]
[23,"设备4_读写M0920","INTEGER","读写00921","读写","[0区]输出继电器","NULL",921]
[24,"设备4_读写M927","INTEGER","读写00927","读写","[0区]输出继电器","NULL",927]
[25,"设备4_读写M0950","INTEGER","读写00951","读写","[0区]输出继电器","NULL",951]
[26,"设备4_读写M0951","INTEGER","读写00952","读写","[0区]输出继电器","NULL",952]
[27,"设备4_读写M0952","INTEGER","读写00953","读写","[0区]输出继电器","NULL",953]
[28,"设备4_读写M0953","INTEGER","读写00954","读写","[0区]输出继电器","NULL",954]
[29,"设备4_读写M0954","INTEGER","读写00955","读写","[0区]输出继电器","NULL",955]
[30,"设备4_读写M0955","INTEGER","读写00956","读写","[0区]输出继电器","NULL",956]
[31,"设备4_读写M0956","INTEGER","读写00957","读写","[0区]输出继电器","NULL",957]
[32,"设备4_读写M0957","INTEGER","读写00958","读写","[0区]输出继电器","NULL",958]
[33,"设备4_读写M0958","INTEGER","读写00959","读写","[0区]输出继电器","NULL",959]
[34,"设备4_读写M0959","INTEGER","读写00960","读写","[0区]输出继电器","NULL",960]
[35,"设备4_读写M0960","INTEGER","读写00961","读写","[0区]输出继电器","NULL",961]
[36,"设备4_读写M0961","INTEGER","读写00962","读写","[0区]输出继电器","NULL",962]
[37,"设备4_读写M0963","INTEGER","读写00964","读写","[0区]输出继电器","NULL",964]
[38,"设备4_读写M0964","INTEGER","读写00965","读写","[0区]输出继电器","NULL",965]
[39,"设备4_读写M0965","INTEGER","读写00966","读写","[0区]输出继电器","NULL",966]
[40,"设备4_读写M0966","INTEGER","读写00967","读写","[0区]输出继电器","NULL",967]
[41,"设备4_读写M0967","INTEGER","读写00968","读写","[0区]输出继电器","NULL",968]
[42,"设备4_读写M0968","INTEGER","读写00969","读写","[0区]输出继电器","NULL",969]
[43,"设备4_读写M0970","INTEGER","读写00971","读写","[0区]输出继电器","NULL",971]
[44,"设备4_读写M0971","INTEGER","读写00972","读写","[0区]输出继电器","NULL",972]
[45,"设备4_读写M1300","INTEGER","读写01301","读写","[0区]输出继电器","NULL",1301]
[46,"设备4_读写M3000","INTEGER","读写03001","读写","[0区]输出继电器","NULL",3001]
[47,"设备4_读写Y0001","INTEGER","读写064514","读写","[0区]输出继电器","NULL",64514]
[48,"设备4_读写Y0002","INTEGER","读写064515","读写","[0区]输出继电器","NULL",64515]
[49,"设备4_读写Y0003","INTEGER","读写064516","读写","[0区]输出继电器","NULL",64516]
[50,"设备4_读写Y0004","INTEGER","读写064517","读写","[0区]输出继电器","NULL",64517]
[51,"设备4_读写Y0005","INTEGER","读写064518","读写","[0区]输出继电器","NULL",64518]
[52,"设备4_读写D160","SINGLE","读写4DB0161","读写","[4区]输出寄存器","32位 有符号二进制",161]
[53,"设备4_读写D184","SINGLE","读写4DF0185","读写","[4区]输出寄存器","32位 浮点数",185]
[54,"设备4_读写D600","SINGLE","读写4DF0601","读写","[4区]输出寄存器","32位 浮点数",601]
[55,"设备4_读写D1000","SINGLE","读写4WUB1001","读写","[4区]输出寄存器","16位 无符号二进制",1001]
[56,"设备4_读写D1001","SINGLE","读写4WUB1002","读写","[4区]输出寄存器","16位 无符号二进制",1002]
[57,"设备4_读写D1002","SINGLE","读写4WUB1003","读写","[4区]输出寄存器","16位 无符号二进制",1003]
[58,"设备4_读写D1003","SINGLE","读写4WUB1004","读写","[4区]输出寄存器","16位 无符号二进制",1004]
[59,"设备4_读写D1184","SINGLE","读写4WUB1185","读写","[4区]输出寄存器","16位 无符号二进制",1185]
[60,"设备4_读写D2000","SINGLE","读写4WUB2001","读写","[4区]输出寄存器","16位 无符号二进制",2001]
[61,"设备4_读写D2002","SINGLE","读写4WUB2003","读写","[4区]输出寄存器","16位 无符号二进制",2003]
[62,"设备4_读写D2003","SINGLE","读写4WUB2004","读写","[4区]输出寄存器","16位 无符号二进制",2004]
[63,"设备4_读写D2004","SINGLE","读写4WUB2005","读写","[4区]输出寄存器","16位 无符号二进制",2005]
[64,"设备4_读写D2022","SINGLE","读写4WB2023","读写","[4区]输出寄存器","16位 有符号二进制",2023]
[65,"设备4_读写D2023","SINGLE","读写4WB2024","读写","[4区]输出寄存器","16位 有符号二进制",2024]
[66,"设备4_读写D2030","SINGLE","读写4WB2031","读写","[4区]输出寄存器","16位 有符号二进制",2031]
[67,"设备4_读写D2034","SINGLE","读写4WUB2035","读写","[4区]输出寄存器","16位 无符号二进制",2035]
[68,"设备4_读写D2040","SINGLE","读写4WUB2041","读写","[4区]输出寄存器","16位 无符号二进制",2041]
[69,"设备4_读写D2050","SINGLE","读写4WUB2051","读写","[4区]输出寄存器","16位 无符号二进制",2051]
[70,"设备4_读写D2058","SINGLE","读写4WB2059","读写","[4区]输出寄存器","16位 有符号二进制",2059]
[71,"设备4_读写D2132","SINGLE","读写4WUB2133","读写","[4区]输出寄存器","16位 无符号二进制",2133]
[72,"设备4_读写D2140","SINGLE","读写4WUB2141","读写","[4区]输出寄存器","16位 无符号二进制",2141]
[73,"设备4_读写D2144","SINGLE","读写4WUB2145","读写","[4区]输出寄存器","16位 无符号二进制",2145]
[74,"设备4_读写D2170","SINGLE","读写4WUB2171","读写","[4区]输出寄存器","16位 无符号二进制",2171]
[75,"设备4_读写D2182","SINGLE","读写4WUB2183","读写","[4区]输出寄存器","16位 无符号二进制",2183]
[76,"设备4_读写D2184","SINGLE","读写4WUB2185","读写","[4区]输出寄存器","16位 无符号二进制",2185]
[77,"设备4_读写D2308","SINGLE","读写4WUB2309","读写","[4区]输出寄存器","16位 无符号二进制",2309]
[78,"设备4_读写D2320","SINGLE","读写4WUB2321","读写","[4区]输出寄存器","16位 无符号二进制",2321]
[79,"设备4_读写D2324","SINGLE","读写4WUB2325","读写","[4区]输出寄存器","16位 无符号二进制",2325]
[80,"设备4_读写D2374","SINGLE","读写4WUB2375","读写","[4区]输出寄存器","16位 无符号二进制",2375]
[81,"设备4_读写D2398","SINGLE","读写4WUB2399","读写","[4区]输出寄存器","16位 无符号二进制",2399]
[82,"设备4_读写D2500","SINGLE","读写4WUB2501","读写","[4区]输出寄存器","16位 无符号二进制",2501]
[83,"设备4_读写D2501","SINGLE","读写4WUB2502","读写","[4区]输出寄存器","16位 无符号二进制",2502]
[84,"设备4_读写D2502","SINGLE","读写4WUB2503","读写","[4区]输出寄存器","16位 无符号二进制",2503]
[85,"设备4_读写D2503","SINGLE","读写4WUB2504","读写","[4区]输出寄存器","16位 无符号二进制",2504]
[86,"设备4_读写D2504","SINGLE","读写4WUB2505","读写","[4区]输出寄存器","16位 无符号二进制",2505]
[87,"设备4_读写D2505","SINGLE","读写4WUB2506","读写","[4区]输出寄存器","16位 无符号二进制",2506]
[88,"设备4_读写D2506","SINGLE","读写4WUB2507","读写","[4区]输出寄存器","16位 无符号二进制",2507]
[89,"设备4_读写D2507","SINGLE","读写4WUB2508","读写","[4区]输出寄存器","16位 无符号二进制",2508]
[90,"设备4_读写D2510","SINGLE","读写4DF2511","读写","[4区]输出寄存器","32位 浮点数",2511]
[91,"设备4_读写D2512","SINGLE","读写4DF2513","读写","[4区]输出寄存器","32位 浮点数",2513]
[92,"设备4_读写D2514","SINGLE","读写4DF2515","读写","[4区]输出寄存器","32位 浮点数",2515]
[93,"设备4_读写D2516","SINGLE","读写4DF2517","读写","[4区]输出寄存器","32位 浮点数",2517]
[94,"设备4_读写D2520","SINGLE","读写4WUB2521","读写","[4区]输出寄存器","16位 无符号二进制",2521]
[95,"设备4_读写D2521","SINGLE","读写4WUB2522","读写","[4区]输出寄存器","16位 无符号二进制",2522]
[96,"设备4_读写D2610","SINGLE","读写4WUB2611","读写","[4区]输出寄存器","16位 无符号二进制",2611]
[97,"设备4_读写D2620","SINGLE","读写4WUB2621","读写","[4区]输出寄存器","16位 无符号二进制",2621]
[98,"设备4_读写D2662","SINGLE","读写4WUB2663","读写","[4区]输出寄存器","16位 无符号二进制",2663]
[99,"设备4_读写D2700","SINGLE","读写4WUB2701","读写","[4区]输出寄存器","16位 无符号二进制",2701]
[100,"设备4_读写D2762","SINGLE","读写4WUB2763","读写","[4区]输出寄存器","16位 无符号二进制",2763]
[101,"设备4_读写D3026","SINGLE","读写4DF3027","读写","[4区]输出寄存器","32位 浮点数",3027]
[102,"设备4_读写D3080","SINGLE","读写4DF3081","读写","[4区]输出寄存器","32位 浮点数",3081]
[103,"设备4_读写D3084","SINGLE","读写4DF3085","读写","[4区]输出寄存器","32位 浮点数",3085]
[104,"设备4_读写D3090","SINGLE","读写4WUB3091","读写","[4区]输出寄存器","16位 无符号二进制",3091]
[105,"设备4_读写D3580","SINGLE","读写4DUB3581","读写","[4区]输出寄存器","32位 无符号二进制",3581]
[106,"设备4_读写D3582","SINGLE","读写4DUB3583","读写","[4区]输出寄存器","32位 无符号二进制",3583]
[107,"设备4_读写D3584","SINGLE","读写4DUB3585","读写","[4区]输出寄存器","32位 无符号二进制",3585]
[108,"设备4_读写D3586","SINGLE","读写4DUB3587","读写","[4区]输出寄存器","32位 无符号二进制",3587]
[109,"设备4_读写D3680","SINGLE","读写4WUB3681","读写","[4区]输出寄存器","16位 无符号二进制",3681]
[110,"设备4_读写D3700","SINGLE","读写4WUB3701","读写","[4区]输出寄存器","16位 无符号二进制",3701]
[111,"设备4_读写D3702","SINGLE","读写4WUB3703","读写","[4区]输出寄存器","16位 无符号二进制",3703]
[112,"设备4_读写D3704","SINGLE","读写4WUB3705","读写","[4区]输出寄存器","16位 无符号二进制",3705]
[113,"设备4_读写D3706","SINGLE","读写4WUB3707","读写","[4区]输出寄存器","16位 无符号二进制",3707]
[114,"设备4_读写D3800","SINGLE","读写4WUB3801","读写","[4区]输出寄存器","16位 无符号二进制",3801]
[115,"设备4_读写D3802","SINGLE","读写4WUB3803","读写","[4区]输出寄存器","16位 无符号二进制",3803]
[116,"设备4_读写D3804","SINGLE","读写4WUB3805","读写","[4区]输出寄存器","16位 无符号二进制",3805]
[117,"设备4_读写D3806","SINGLE","读写4WUB3807","读写","[4区]输出寄存器","16位 无符号二进制",3807]
[118,"设备4_读写D4026","SINGLE","读写4DF4027","读写","[4区]输出寄存器","32位 浮点数",4027]
[119,"设备4_读写D4080","SINGLE","读写4DF4081","读写","[4区]输出寄存器","32位 浮点数",4081]
[120,"设备4_读写D4084","SINGLE","读写4DF4085","读写","[4区]输出寄存器","32位 浮点数",4085]
[121,"设备4_读写D4090","SINGLE","读写4WUB4091","读写","[4区]输出寄存器","16位 无符号二进制",4091]
[122,"设备4_读写D5026","SINGLE","读写4DF5027","读写","[4区]输出寄存器","32位 浮点数",5027]
[123,"设备4_读写D5080","SINGLE","读写4DF5081","读写","[4区]输出寄存器","32位 浮点数",5081]
[124,"设备4_读写D5084","SINGLE","读写4DF5085","读写","[4区]输出寄存器","32位 浮点数",5085]
[125,"设备4_读写D5090","SINGLE","读写4WUB5091","读写","[4区]输出寄存器","16位 无符号二进制",5091]
[126,"设备4_读写D6012","SINGLE","读写4DF6013","读写","[4区]输出寄存器","32位 浮点数",6013]
[127,"设备4_读写D6026","SINGLE","读写4DF6027","读写","[4区]输出寄存器","32位 浮点数",6027]
[128,"设备4_读写D6080","SINGLE","读写4DF6081","读写","[4区]输出寄存器","32位 浮点数",6081]
[129,"设备4_读写D6084","SINGLE","读写4DF6085","读写","[4区]输出寄存器","32位 浮点数",6085]
[130,"设备4_读写D6090","SINGLE","读写4WUB6091","读写","[4区]输出寄存器","16位 无符号二进制",6091]
[131,"设备4_读写D6300","SINGLE","读写4DF6301","读写","[4区]输出寄存器","32位 浮点数",6301]
[132,"设备4_读写D6304","SINGLE","读写4DF6305","读写","[4区]输出寄存器","32位 浮点数",6305]
[133,"设备4_读写D6308","SINGLE","读写4DF6309","读写","[4区]输出寄存器","32位 浮点数",6309]
[134,"设备4_读写D6312","SINGLE","读写4DF6313","读写","[4区]输出寄存器","32位 浮点数",6313]
[135,"设备4_读写D6316","SINGLE","读写4DF6317","读写","[4区]输出寄存器","32位 浮点数",6317]
[136,"设备4_读写D6320","SINGLE","读写4DF6321","读写","[4区]输出寄存器","32位 浮点数",6321]
[137,"设备4_读写D6322","SINGLE","读写4DF6323","读写","[4区]输出寄存器","32位 浮点数",6323]
[138,"设备4_读写D6324","SINGLE","读写4DF6325","读写","[4区]输出寄存器","32位 浮点数",6325]
[139,"设备4_读写D6326","SINGLE","读写4DF6327","读写","[4区]输出寄存器","32位 浮点数",6327]
[140,"设备4_读写D6328","SINGLE","读写4DF6329","读写","[4区]输出寄存器","32位 浮点数",6329]
[141,"设备4_读写D6330","SINGLE","读写4DF6331","读写","[4区]输出寄存器","32位 浮点数",6331]
[142,"设备4_读写D6332","SINGLE","读写4DF6333","读写","[4区]输出寄存器","32位 浮点数",6333]
[143,"设备4_读写D6334","SINGLE","读写4DF6335","读写","[4区]输出寄存器","32位 浮点数",6335]
[144,"设备4_读写D6336","SINGLE","读写4DF6337","读写","[4区]输出寄存器","32位 浮点数",6337]