{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["参数","地址段映射","设备地址"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"参数","index":0,"n_rows":90,"n_cols":7,"rows_kept":90,"cut":false,"hidden":false,"merged":[]}
["界面","描述","属性名","类型","放大","可写","HMI寄存器"]
["风机控制","进风指示","IsInletAirOn","bool",null,"Y","设备0.Y(1)"]
["风机控制","进风运行频率(Hz)(自动调节)","InletAirFreq","uint16",0.1,null,"设备0.D(6120)"]
["风机控制","进风设定频率(Hz)","InletAirFreqSet","uint16",0.1,"Y","设备0.D(3200)"]
["风机控制","出风指示","IsOutletAirOn","bool",null,"Y","设备0.Y(2)"]
["风机控制","出风运行频率(Hz)","OutletAirFreq","uint16",0.1,null,"设备0.D(6220)"]
["风机控制","出风设定频率(Hz)","OutletAirFreqSet","uint16",0.1,"Y","设备0.D(592)"]
["风机控制","出风设定频率后通知","IsOutletAirFreqChanged","bool",null,"Y","设备0.M(99)"]
["风机控制","折径显示(mm)","FilmWidth","uint16",null,null,"设备0.D(668)"]
["风机控制","折径设定(mm)","FilmWidthSet","uint16",null,"Y","设备0.D(230)"]
["风机控制","折径设定后通知","IsFilmWidthChanged","bool",null,"Y","设备0.M(800)"]
["风机控制","误差校正","ErrorCorrection","int16",null,"Y","设备0.D(340)"]
["风机控制","IBC自动","IsIBCAuto","bool",null,"Y","设备0.M(659)"]
["风机控制","外冷指示","IsExCoolOn","bool",null,"Y","设备0.M(178)"]
["风机控制","外冷运行频率(Hz)","ExCoolFreq","uint16",0.1,null,"设备0.D(5050)"]
["风机控制","外冷设定频率(Hz)","ExCoolFreqSet","uint16",0.1,"Y","设备0.D(5000)"]
["膜泡校正","K1","K1","uint16",null,null,"设备0.D(1140)"]
["膜泡校正","K2","K2","uint16",null,null,"设备0.D(1142)"]
["膜泡校正","K3","K3","uint16",null,null,"设备0.D(1144)"]
["膜泡校正","L","L","float",null,"Y","设备0.D(250)"]
["膜泡校正","膜泡校正A","BubbleCorrA","float",null,null,"设备0.D(18)"]
["膜泡校正","膜泡校正B","BubbleCorrB","float",null,null,"设备0.D(28)"]
["膜泡校正","膜泡校正C","BubbleCorrC","float",null,null,"设备0.D(38)"]
["膜泡校正","膜泡校正R","BubbleCorrR","float",null,null,"设备0.D(102)"]
["IBC系统参数","采样周期","SampleInterval","uint16",0.1,"Y","设备0.D(300)"]
["IBC系统参数","区间1设置","Area1Set","uint16",null,"Y","设备0.D(304)"]
["IBC系统参数","区间1P","Area1P","uint16",null,"Y","设备0.D(1001)"]
["IBC系统参数","区间1I","Area1I","uint16",null,"Y","设备0.D(1002)"]
["IBC系统参数","区间1D","Area1D","uint16",null,"Y","设备0.D(1003)"]
["IBC系统参数","区间1DI","Area1DI","uint16",null,"Y","设备0.D(1004)"]
["IBC系统参数","调节系数","AdjustFactor","uint16",0.01,"Y","设备0.D(2550)"]
["IBC系统参数","PID结果","PIDResult","int16",null,null,"设备0.D(2050)"]
["IBC系统参数","PID调节","PIDAdjust","int16",null,null,"设备0.D(2052)"]
["IBC系统参数","进风速度","InletAirVelocity","uint16",null,null,"设备0.D(710)"]
["IBC系统参数","出风速度","OutletAirVelocity","uint16",null,null,"设备0.D(712)"]
["IBC系统参数","速度系数","VelocityFactor","float",null,"Y","设备0.D(3502)"]
["IBC系统参数","牵引直径","TractionDiameter","float",null,"Y","设备0.D(3504)"]
["IBC系统参数","牵引速比","TractionVRatio","float",null,"Y","设备0.D(3506)"]
["IBC系统参数","牵引速度(内部）","TractionVelocityInner","uint16",null,null,"设备0.D(3524)"]
["IBC系统参数2","区间2设置","Area2Set","uint16",null,"Y","设备0.D(306)"]
["IBC系统参数2","区间2P","Area2P","uint16",null,"Y","设备0.D(1201)"]
["IBC系统参数2","区间2I","Area2I","uint16",null,"Y","设备0.D(1202)"]
["IBC系统参数2","区间2D","Area2D","uint16",null,"Y","设备0.D(1203)"]
["IBC系统参数2","传感器1盲区","Sensor1DeadZone","float",null,"Y","设备0.D(420)"]
["IBC系统参数2","传感器2盲区","Sensor2DeadZone","float",null,"Y","设备0.D(430)"]
["IBC系统参数2","传感器3盲区","Sensor3DeadZone","float",null,"Y","设备0.D(440)"]
["IBC系统参数2","传感器1系数","Sensor1Factor","float",null,"Y","设备0.D(200)"]
["IBC系统参数2","传感器2系数","Sensor2Factor","float",null,"Y","设备0.D(400)"]
["IBC系统参数2","传感器3系数","Sensor3Factor","float",null,"Y","设备0.D(410)"]
["IBC系统参数2","外冷额定频率","ExCoolDefaultFreq","uint16",0.1,"Y","设备0.D(5004)"]
["IBC系统参数2","出风额定频率","OutletAirDefaultFreq","uint16",0.1,"Y","设备0.D(5012)"]
["IBC系统参数2","进风额定频率","InletAirDefaultFreq","uint16",0.1,"Y","设备0.D(5010)"]
["IBC系统参数2","牵引额定频率","TractionDefaultFreq","uint16",0.1,"Y","设备0.D(3580)"]
["IBC系统参数2","旋转额定频率","RotationDefaultFreq","uint16",0.1,"Y","设备0.D(5104)"]
["螺杆","牵引速度","TractionVelocity","float",null,null,"设备0.D(3542)"]
["螺杆","牵引速度设置","TractionVelocitySet","float",null,"Y","设备0.D(3500)"]
["螺杆","主牵引运行指示","IsTractionOn","bool",null,null,"设备0.M(177)"]
["螺杆","主牵引开","TractionOn","bool",null,"Y","设备0.M(176)"]
["螺杆","气垫辊风机运行指示","IsAirCushionOn","bool",null,null,"设备0.Y(5)"]
["螺杆","气垫辊风机开","AirCushionOn","bool",null,"Y","设备0.M(34)"]
["旋转塔","旋转塔正转指示","IsRotaryForw","bool",null,null,"设备0.M(180)"]
["旋转塔","旋转塔反转指示","IsRotaryBackw","bool",null,null,"设备0.M(181)"]
["旋转塔","旋转塔正转","RotaryForw","bool",null,null,"设备0.M(500)"]
["旋转塔","旋转塔反转","RotaryBackw","bool",null,null,"设备0.M(501)"]
["旋转塔","旋转塔正向机械限位","IsRotaryForwLimit","bool",null,null,"设备0.X(3)"]
["旋转塔","旋转塔正转换向限位","IsRotaryForwTurn","bool",null,null,"设备0.X(2)"]
["旋转塔","旋转塔复位原点限位","IsRotaryOrgSign","bool",null,null,"设备0.X(6)"]
["旋转塔","旋转塔反转换向限位","IsRotaryBackwTurn","bool",null,null,"设备0.X(4)"]
["旋转塔","旋转塔反向机械限位","IsRotaryBackwLimit","bool",null,null,"设备0.X(5)"]
["旋转塔","旋转塔电机频率设定(Hz)","RotaryFreqSet","uint16",0.1,"Y","设备0.D(5100)"]
["旋转塔","旋转塔电机频率显示(Hz)","RotaryFreq","uint16",0.1,null,"设备0.D(5120)"]
["旋转塔","旋转塔复位指示","IsRotaryOrg","bool",null,"Y","M(414)"]
["旋转塔","旋转塔复位(┷）","RotaryOrg","bool",null,"Y","M(413)"]
["旋转塔","旋转塔开启指示","IsRotaryOn","bool",null,"Y","M(411)"]
["旋转塔","旋转塔开启(┷）","RotaryOn","bool",null,"Y","M(416)"]
["报警","故障复位","AlarmReset","bool",null,"Y","设备0.M(63)"]
["报警","进风变频故障报警","IsInletAirMotorError","bool",null,null,"设备0.M(60)"]
["报警","出风变频故障报警","IsOutletAirMotorError","bool",null,null,"设备0.M(61)"]
["报警","进风变频通讯报警","IsInletAirCommError","bool",null,null,"设备0.M(403)"]
["报警","出风变频通讯报警","IsOutletAirCommError","bool",null,null,"设备0.M(404)"]
["报警","外冷变频故障报警","IsExCoolMotorError","bool",null,null,"设备0.M(64)"]
["报警","旋转变频故障报警","IsRotationMotorError","bool",null,null,"设备0.M(68)"]
["报警","牵引变频故障报警","IsTractionMotorError","bool",null,null,"设备0.M(69)"]
["报警","外冷变频通讯报警","IsExCoolCommError","bool",null,null,"设备0.M(405)"]
["报警","旋转变频通讯报警","IsRotationCommError","bool",null,null,"设备0.M(409)"]
["报警","牵引变频通讯报警","IsTractionCommError","bool",null,null,"设备0.M(430)"]
["报警","风机电源报警","IsAirPowerError","bool",null,null,"设备0.X(15)"]
["报警","急停开启报警","IsEmergencyStopError","bool",null,null,"设备0.X(16)"]
["报警","旋转正转极限报警","IsRotationForwLimitError","bool",null,null,"设备0.M(1202)"]
["报警","旋转反转极限报警","IsRotationBackwLimitError","bool",null,null,"设备0.M(1203)"]

{"sheet":"地址段映射","index":1,"n_rows":5,"n_cols":4,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
["PLC寄存器类型","PLC寄存器首地址","MB寄存器类型","MB寄存器首地址"]
["D",0,"[4区]输出寄存器",1]
["M",0,"[0区]输出继电器",1]
["Y",0,"[0区]输出继电器",64513]
["X",0,"[1区]输入继电器",63489]

{"sheet":"设备地址","index":2,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["设备序号","EP"]
[0,"192.168.50.30:502"]