{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["类表","设备地址","地址段映射","地址格式","各层参数","参数"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"类表","index":0,"n_rows":3,"n_cols":4,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["类名","表名","单例","实例名"]
["WeighterC","各层参数","N","Items"]
["WeighterAccessory","参数","Y","Accessory"]

{"sheet":"设备地址","index":1,"n_rows":6,"n_cols":2,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
["设备名称","EP"]
["设备1","192.168.50.2:502"]
["设备0","192.168.50.1:502"]
["设备2","192.168.50.3:502"]
["设备3","192.168.50.4:502"]
["设备4","192.168.50.5:502"]

{"sheet":"地址段映射","index":2,"n_rows":7,"n_cols":5,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["PLC寄存器类型","MB寄存器类型","MB寄存器首地址","进制"]
["D","[4区]输出寄存器","0x0",10,0]
["M","[0区]输出继电器","0x0",10,0]
["Y","[0区]输出继电器","0xFC00",8,64512]
["X","[1区]输入继电器","0xF800",8,63488]
["S","[1区]输入继电器","0xE000",10,57344]
["R","[4区]输出寄存器","0x3000",10,12288]

{"sheet":"地址格式","index":3,"n_rows":5,"n_cols":4,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
["正则表达式","设备名称Group序号","寄存器类型Group序号","地址Group序号"]
["\\A([\\w]+)_(?:读写|只读)(\\w)(\\d+)\\z",1,2,3]
[]
[]
["设备1_读写D2507"]

{"sheet":"各层参数","index":4,"n_rows":145,"n_cols":13,"rows_kept":145,"cut":false,"hidden":false,"merged":[]}
["界面","描述","属性名","类型","放大","可写","报警","触发","A层HMI寄存器","B层HMI寄存器","C层HMI寄存器","D层HMI寄存器","E层HMI寄存器"]
["主界面","报警开关","AlarmIsOn","bool",null,"Y",null,null,"设备1_读写M0970","设备0_读写M0970","设备2_读写M0970","设备3_读写M0970","设备4_读写M0970"]
["主界面","报警复位","IsAlarmReseted","bool",null,"Y",null,null,"设备1_读写M0971","设备0_读写M0971","设备2_读写M0971","设备3_读写M0971","设备4_读写M0971"]
["主界面","累计产量","CumulativeProduction","float",null,null,null,null,"设备1_读写D6320","设备0_读写D6320","设备2_读写D6320","设备3_读写D6320","设备4_读写D6320"]
["主界面","配料斗重量显示","MixBucketWeight","float",null,null,null,null,"设备1_读写D184","设备0_读写D184","设备2_读写D184","设备3_读写D184","设备4_读写D184"]
["主界面","配料斗阀门","BucketValveIsOpen","bool",null,"Y",null,null,"设备1_读写M0020","设备0_读写M0020","设备2_读写M0020","设备3_读写M0020","设备4_读写M0020"]
["主界面","配料操作","MixIsOn","bool",null,"Y",null,null,"设备1_读写M0035","设备0_读写M0035","设备2_读写M0035","设备3_读写M0035","设备4_读写M0035"]
["主界面","失重仓重量","BinWeight","Int32",0.001,null,null,null,"设备1_读写D160","设备0_读写D160","设备2_读写D160","设备3_读写D160","设备4_读写D160"]
["主界面","当前产量","CurrentFlow","UInt16",0.1,null,null,null,"设备1_读写D2398","设备0_读写D2398","设备2_读写D2398","设备3_读写D2398","设备4_读写D2398"]
["主界面","设定产量","FlowSetting","UInt16",0.1,null,null,null,"设备1_读写D2144","设备0_读写D2144","设备2_读写D2144","设备3_读写D2144","设备4_读写D2144"]
["主界面","运行比例","ScrewPDisp","UInt16",0.1,null,null,null,"设备1_读写D3702","设备1_读写D3704","设备1_读写D3706","设备1_读写D3710","设备1_读写D3712"]
["主界面","设定比例","ScrewPSet","UInt16",0.1,"Y",null,null,"设备1_读写D3802","设备1_读写D3804","设备1_读写D3806","设备1_读写D3830","设备1_读写D3832"]
["主界面","运行频率","ScrewMotorFreq","UInt16",0.1,null,null,null,"设备1_读写D2320","设备0_读写D2320","设备2_读写D2320","设备3_读写D2320","设备4_读写D2320"]
["主界面","设定频率","ScrewManualFreq","float",null,"Y",null,null,"设备1_读写D1700","设备0_读写D1700","设备2_读写D1700","设备3_读写D1700","设备4_读写D1700"]
["主界面","设定频率确定","ScrewManualFreqIsSet","bool",null,"Y",null,null,"设备1_读写M0350","设备0_读写M0350","设备2_读写M0350","设备3_读写M0350","设备4_读写M0350"]
["主界面","螺杆模式","ScrewIsAutoMode","bool",null,"Y",null,null,"设备1_读写M0910","设备0_读写M0910","设备2_读写M0910","设备3_读写M0910","设备4_读写M0910"]
["主界面","螺杆操作","ScrewMotorIsOn","bool",null,"Y",null,null,"设备1_读写M0150","设备0_读写M0150","设备2_读写M0150","设备3_读写M0150","设备4_读写M0150"]
["配置画面","1#比例设定","MixPSet_1","UInt16",0.1,"Y",null,null,"设备1_读写D1001","设备0_读写D1000","设备2_读写D1001","设备3_读写D1000","设备4_读写D1000"]
["配置画面","2#比例设定","MixPSet_2","UInt16",0.1,"Y",null,null,"设备1_读写D1002","设备0_读写D1001","设备2_读写D1002","设备3_读写D1001","设备4_读写D1001"]
["配置画面","3#比例设定","MixPSet_3","UInt16",0.1,"Y",null,null,"设备1_读写D1003","设备0_读写D1002","设备2_读写D1003","设备3_读写D1002","设备4_读写D1002"]
["配置画面","4#比例设定","MixPSet_4","UInt16",0.1,"Y",null,null,"设备1_读写D1004","设备0_读写D1003","设备2_读写D1004","设备3_读写D1003","设备4_读写D1003"]
["配置画面","5#比例设定","MixPSet_5","UInt16",0.1,"Y",null,null,"设备1_读写D1005",null,"设备2_读写D1005",null,"设备4_读写D1004"]
["配置画面","6#比例设定","MixPSet_6","UInt16",0.1,"Y",null,null,null,null,null,null,"设备4_读写D1005"]
["配置画面","1#比例显示","MixPDisp_1","float",null,null,null,null,"设备1_读写D6308","设备0_读写D6304","设备2_读写D6308","设备3_读写D6304","设备4_读写D6304"]
["配置画面","2#比例显示","MixPDisp_2","float",null,null,null,null,"设备1_读写D6312","设备0_读写D6308","设备2_读写D6312","设备3_读写D6308","设备4_读写D6308"]
["配置画面","3#比例显示","MixPDisp_3","float",null,null,null,null,"设备1_读写D6316","设备0_读写D6312","设备2_读写D6316","设备3_读写D6312","设备4_读写D6312"]
["配置画面","4#比例显示","MixPDisp_4","float",null,null,null,null,"设备1_读写R6304","设备0_读写D6316","设备2_读写R6304","设备3_读写D6316","设备4_读写D6316"]
["配置画面","5#比例显示","MixPDisp_5","float",null,null,null,null,"设备1_读写R6308",null,"设备2_读写R6308",null,"设备4_读写R6304"]
["配置画面","6#比例显示","MixPDisp_6","float",null,null,null,null,null,null,null,null,"设备4_读写R6308"]
["配置画面","1#重量设定","MixSet_1","float",null,null,null,null,"设备1_读写D5080","设备0_读写D6080","设备2_读写D5080","设备3_读写D6080","设备4_读写D6080"]
["配置画面","2#重量设定","MixSet_2","float",null,null,null,null,"设备1_读写D4080","设备0_读写D5080","设备2_读写D4080","设备3_读写D5080","设备4_读写D5080"]
["配置画面","3#重量设定","MixSet_3","float",null,null,null,null,"设备1_读写D3080","设备0_读写D4080","设备2_读写D3080","设备3_读写D4080","设备4_读写D4080"]
["配置画面","4#重量设定","MixSet_4","float",null,null,null,null,"设备1_读写R6080","设备0_读写D3080","设备2_读写R6080","设备3_读写D3080","设备4_读写D3080"]
["配置画面","5#重量设定","MixSet_5","float",null,null,null,null,"设备1_读写R5080",null,"设备2_读写R5080",null,"设备4_读写R6080"]
["配置画面","6#重量设定","MixSet_6","float",null,null,null,null,null,null,null,null,"设备4_读写R5080"]
["配置画面","1#重量显示","MixDisp_1","float",null,null,null,null,"设备1_读写D5084","设备0_读写D6084","设备2_读写D5084","设备3_读写D6084","设备4_读写D6084"]
["配置画面","2#重量显示","MixDisp_2","float",null,null,null,null,"设备1_读写D4084","设备0_读写D5084","设备2_读写D4084","设备3_读写D5084","设备4_读写D5084"]
["配置画面","3#重量显示","MixDisp_3","float",null,null,null,null,"设备1_读写D3084","设备0_读写D4084","设备2_读写D3084","设备3_读写D4084","设备4_读写D4084"]
["配置画面","4#重量显示","MixDisp_4","float",null,null,null,null,"设备1_读写R6084","设备0_读写D3084","设备1_读写R6084","设备3_读写D3084","设备4_读写D3084"]
["配置画面","5#重量显示","MixDisp_5","float",null,null,null,null,"设备1_读写R5084",null,"设备1_读写R5084",null,"设备4_读写R6084"]
["配置画面","6#重量显示","MixDisp_6","float",null,null,null,null,null,null,null,null,"设备4_读写R5084"]
["配置画面","1#放料","MixLight_1","bool",null,null,null,null,"设备1_读写Y0002","设备0_读写Y0001","设备2_读写Y0002","设备3_读写Y0001","设备4_读写Y0001"]
["配置画面","2#放料","MixLight_2","bool",null,null,null,null,"设备1_读写Y0003","设备0_读写Y0002","设备2_读写Y0003","设备3_读写Y0002","设备4_读写Y0002"]
["配置画面","3#放料","MixLight_3","bool",null,null,null,null,"设备1_读写Y0004","设备0_读写Y0003","设备2_读写Y0004","设备3_读写Y0003","设备4_读写Y0003"]
["配置画面","4#放料","MixLight_4","bool",null,null,null,null,"设备1_读写Y0011","设备0_读写Y0004","设备2_读写Y0011","设备3_读写Y0004","设备4_读写Y0004"]
["配置画面","5#放料","MixLight_5","bool",null,null,null,null,"设备1_读写Y0012",null,"设备2_读写Y0012",null,"设备4_读写Y0011"]
["配置画面","6#放料","MixLight_6","bool",null,null,null,null,null,null,null,null,"设备4_读写Y0012"]
["配置画面","配料斗卸载","MixUnload","bool",null,null,null,null,"设备1_读写Y0005","设备0_读写Y0005","设备2_读写Y0005","设备3_读写Y0005","设备4_读写Y0005"]
["配置画面","配料斗重量设置","MixSet","float",null,"Y",null,null,"设备1_读写D6012","设备0_读写D6012","设备2_读写D6012","设备3_读写D6012","设备4_读写D6012"]
["配置画面","配料斗重量显示","MixDisp","float",null,null,null,null,"设备1_读写D6300","设备0_读写D6300","设备2_读写D6300","设备3_读写D6300","设备4_读写D6300"]
["配置画面","1#累计重量","MixCum_1","float",null,null,null,null,"设备1_读写D6326","设备0_读写D6322","设备2_读写D6326","设备3_读写D6322","设备4_读写D6322"]
["配置画面","2#累计重量","MixCum_2","float",null,null,null,null,"设备1_读写D6330","设备0_读写D6326","设备2_读写D6330","设备3_读写D6326","设备4_读写D6326"]
["配置画面","3#累计重量","MixCum_3","float",null,null,null,null,"设备1_读写D6334","设备0_读写D6330","设备2_读写D6334","设备3_读写D6330","设备4_读写D6330"]
["配置画面","4#累计重量","MixCum_4","float",null,null,null,null,"设备1_读写R6322","设备0_读写D6334","设备2_读写R6322","设备3_读写D6334","设备4_读写D6334"]
["配置画面","5#累计重量","MixCum_5","float",null,null,null,null,"设备1_读写R6326",null,"设备2_读写R6326",null,"设备4_读写R6322"]
["配置画面","6#累计重量","MixCum_6","float",null,null,null,null,null,null,null,null,"设备4_读写R6326"]
["配置画面","1#累计百分比","MixCumPercent_1","float",null,null,null,null,"设备1_读写D6328","设备0_读写D6324","设备2_读写D6328","设备3_读写D6324","设备4_读写D6324"]
["配置画面","2#累计百分比","MixCumPercent_2","float",null,null,null,null,"设备1_读写D6332","设备0_读写D6328","设备2_读写D6332","设备3_读写D6328","设备4_读写D6328"]
["配置画面","3#累计百分比","MixCumPercent_3","float",null,null,null,null,"设备1_读写D6336","设备0_读写D6332","设备2_读写D6336","设备3_读写D6332","设备4_读写D6332"]
["配置画面","4#累计百分比","MixCumPercent_4","float",null,null,null,null,"设备1_读写R6324","设备0_读写D6336","设备2_读写R6324","设备3_读写D6336","设备4_读写D6336"]
["配置画面","5#累计百分比","MixCumPercent_5","float",null,null,null,null,"设备1_读写R6328",null,"设备2_读写R6328",null,"设备4_读写R6324"]
["配置画面","6#累计百分比","MixCumPercent_6","float",null,null,null,null,null,null,null,null,"设备4_读写R6328"]
["配置画面","产量清零","ClearProduction","bool",null,"Y",null,null,"设备1_读写M0156","设备0_读写M0156","设备2_读写M0156","设备3_读写M0156","设备4_读写M0156"]
["螺杆参数","流量方式","FlowCalMethodIsA","bool",null,"Y",null,null,"设备1_读写M3000","设备0_读写M3000","设备2_读写M3000","设备3_读写M3000","设备4_读写M3000"]
["螺杆参数","流量反馈","FlowDisp","UInt16",0.1,null,null,null,"设备1_读写D2170","设备0_读写D2170","设备2_读写D2170","设备3_读写D2170","设备4_读写D2170"]
["螺杆参数","滤波系数设定","FilterParam","UInt16",0.1,"Y",null,null,"设备1_读写D2002","设备0_读写D2002","设备2_读写D2002","设备3_读写D2002","设备4_读写D2002"]
["螺杆参数","切换级别设定","SwitchLv","UInt16",0.1,"Y",null,null,"设备1_读写D2610","设备0_读写D2610","设备2_读写D2610","设备3_读写D2610","设备4_读写D2610"]
["螺杆参数","升降增益设定","UpDownGain","UInt16",0.01,"Y",null,null,"设备1_读写D2040","设备0_读写D2040","设备2_读写D2040","设备3_读写D2040","设备4_读写D2040"]
["螺杆参数","比例增益设定","PGain","UInt16",0.01,"Y",null,null,"设备1_读写D2034","设备0_读写D2034","设备2_读写D2034","设备3_读写D2034","设备4_读写D2034"]
["螺杆参数","积分时间设定","ITime","UInt16",null,"Y",null,null,"设备1_读写D2004","设备0_读写D2004","设备2_读写D2004","设备3_读写D2004","设备4_读写D2004"]
["螺杆参数","调节系数设定","AdjustFactor","UInt16",0.01,"Y",null,null,"设备1_读写D2050","设备0_读写D2050","设备2_读写D2050","设备3_读写D2050","设备4_读写D2050"]
["螺杆参数","调节上限设定","AdjustUpper","Int16",null,"Y",null,null,"设备1_读写D2022","设备0_读写D2022","设备2_读写D2022","设备3_读写D2022","设备4_读写D2022"]
["螺杆参数","调节下限设定","AdjustLower","Int16",null,"Y",null,null,"设备1_读写D2023","设备0_读写D2023","设备2_读写D2023","设备3_读写D2023","设备4_读写D2023"]
["螺杆参数","稳定级别切换","StableLvSwitch","UInt16",0.1,"Y",null,null,"设备1_读写D2662","设备0_读写D2662","设备2_读写D2662","设备3_读写D2662","设备4_读写D2662"]
["螺杆参数","PID调节限幅","PIDLimit","UInt16",null,"Y",null,null,"设备1_读写D2762","设备0_读写D2762","设备2_读写D2762","设备3_读写D2762","设备4_读写D2762"]
["螺杆参数","采样时间","SampleTime","UInt16",null,null,null,null,"设备1_读写D2000","设备0_读写D2000","设备2_读写D2000","设备3_读写D2000","设备4_读写D2000"]
["螺杆参数","PID结果","PIDResult","Int16",null,null,null,null,"设备1_读写D2030","设备0_读写D2030","设备2_读写D2030","设备3_读写D2030","设备4_读写D2030"]
["螺杆参数","PID调节","PIDAdjust","Int16",null,null,null,null,"设备1_读写D2058","设备0_读写D2058","设备2_读写D2058","设备3_读写D2058","设备4_读写D2058"]
["螺杆参数","实际速度","ScrewCurrentSpeed","UInt16",null,null,null,null,"设备1_读写D2700","设备0_读写D2700","设备2_读写D2700","设备3_读写D2700","设备4_读写D2700"]
["螺杆参数","比例增益","PGainDisp","UInt16",0.01,null,null,null,"设备1_读写D2003","设备0_读写D2003","设备2_读写D2003","设备3_读写D2003","设备4_读写D2003"]
["参数设置","卸料时间","UnloadingTime","UInt16",0.1,"Y",null,null,"设备1_读写D2520","设备0_读写D2520","设备2_读写D2520","设备3_读写D2520","设备4_读写D2520"]
["参数设置","零位稳定时间","ZeroStableTime","UInt16",0.1,"Y",null,null,"设备1_读写D2521","设备0_读写D2521","设备2_读写D2521","设备3_读写D2521","设备4_读写D2521"]
["参数设置","流量切换允许","FlowSwitchEnable","UInt16",0.1,"Y",null,null,"设备1_读写D2374","设备0_读写D2374","设备2_读写D2374","设备3_读写D2374","设备4_读写D2374"]
["参数设置","取样时间设定(s)","SampleTimeSet","UInt16",0.1,"Y",null,null,"设备1_读写D2132","设备0_读写D2132","设备2_读写D2132","设备3_读写D2132","设备4_读写D2132"]
["参数设置","额定频率(Hz)","ScrewMotorRatedFreq","UInt16",0.1,"Y",null,null,"设备1_读写D2324","设备0_读写D2324","设备2_读写D2324","设备3_读写D2324","设备4_读写D2324"]
["参数设置","重量稳定时间(s)","WeightStableTime","UInt16",0.1,"Y",null,null,"设备1_读写D1184","设备0_读写D1184","设备2_读写D1184","设备3_读写D1184","设备4_读写D1184"]
["参数设置","料位下限设定(kg)","MaterialLowLimitSet","UInt16",0.1,"Y",null,null,"设备1_读写D2182","设备0_读写D2182","设备2_读写D2182","设备3_读写D2182","设备4_读写D2182"]
["参数设置","报警偏差设定(%)","AlarmDeviationSet","UInt16",null,"Y",null,null,"设备1_读写D2140","设备0_读写D2140","设备2_读写D2140","设备3_读写D2140","设备4_读写D2140"]
["参数设置","重量校正系数","WeightCorrectFactor","UInt16",0.01,"Y",null,null,"设备1_读写D2620","设备0_读写D2620","设备2_读写D2620","设备3_读写D2620","设备4_读写D2620"]
["参数设置","缺料报警设定(kg)","LackErrorSet","UInt16",0.1,"Y",null,null,"设备1_读写D2184","设备0_读写D2184","设备2_读写D2184","设备3_读写D2184","设备4_读写D2184"]
["参数设置","搅拌时间设定(s)","MixingTimeSet","UInt16",0.1,"Y",null,null,"设备1_读写D3680","设备0_读写D3680","设备2_读写D3680","设备3_读写D3680","设备4_读写D3680"]
["配料参数","1次补料偏差","FeedingDeviation_1","float",null,"Y",null,null,"设备1_读写D2510","设备0_读写D2510","设备2_读写D2510","设备3_读写D2510","设备4_读写D2510"]
["配料参数","2次补料偏差","FeedingDeviation_2","float",null,"Y",null,null,"设备1_读写D2512","设备0_读写D2512","设备2_读写D2512","设备3_读写D2512","设备4_读写D2512"]
["配料参数","3次补料偏差","FeedingDeviation_3","float",null,"Y",null,null,"设备1_读写D2514","设备0_读写D2514","设备2_读写D2514","设备3_读写D2514","设备4_读写D2514"]
["配料参数","4次补料偏差","FeedingDeviation_4","float",null,"Y",null,null,"设备1_读写D2516","设备0_读写D2516","设备2_读写D2516","设备3_读写D2516","设备4_读写D2516"]
["配料参数","5次补料偏差","FeedingDeviation_5","float",null,"Y",null,null,"设备1_读写R2510",null,"设备2_读写R2510",null,"设备4_读写R2510"]
["配料参数","6次补料偏差","FeedingDeviation_6","float",null,"Y",null,null,null,null,null,null,"设备4_读写R2512"]
["配料参数","1次加料设定","FeedSet_1","float",null,"Y",null,null,"设备1_读写D6026","设备0_读写D6026","设备2_读写D6026","设备3_读写D6026","设备4_读写D6026"]
["配料参数","2次加料设定","FeedSet_2","float",null,"Y",null,null,"设备1_读写D5026","设备0_读写D5026","设备2_读写D5026","设备3_读写D5026","设备4_读写D5026"]
["配料参数","3次加料设定","FeedSet_3","float",null,"Y",null,null,"设备1_读写D4026","设备0_读写D4026","设备2_读写D4026","设备3_读写D4026","设备4_读写D4026"]
["配料参数","4次加料设定","FeedSet_4","float",null,"Y",null,null,"设备1_读写D3026","设备0_读写D3026","设备2_读写D3026",null,"设备4_读写D3026"]
["配料参数","5次加料设定","FeedSet_5","float",null,"Y",null,null,"设备1_读写R6026",null,"设备2_读写R6026",null,"设备4_读写R6026"]
["配料参数","6次加料设定","FeedSet_6","float",null,"Y",null,null,null,null,null,null,"设备4_读写R5026"]
["配料参数","1#初始时间","InitTime_1","UInt16",0.1,"Y",null,null,"设备1_读写D2500","设备0_读写D2500","设备2_读写D2500","设备3_读写D2500","设备4_读写D2500"]
["配料参数","2#初始时间","InitTime_2","UInt16",0.1,"Y",null,null,"设备1_读写D2501","设备0_读写D2501","设备2_读写D2501","设备3_读写D2501","设备4_读写D2501"]
["配料参数","3#初始时间","InitTime_3","UInt16",0.1,"Y",null,null,"设备1_读写D2502","设备0_读写D2502","设备2_读写D2502","设备3_读写D2502","设备4_读写D2502"]
["配料参数","4#初始时间","InitTime_4","UInt16",0.1,"Y",null,null,"设备1_读写D2503","设备0_读写D2503","设备2_读写D2503","设备3_读写D2503","设备4_读写D2503"]
["配料参数","5#初始时间","InitTime_5","UInt16",0.1,"Y",null,null,"设备1_读写R2501",null,"设备2_读写R2501",null,"设备4_读写R2500"]
["配料参数","6#初始时间","InitTime_6","UInt16",0.1,"Y",null,null,null,null,null,null,"设备4_读写R2501"]
["配料参数","1#最小时间","MinTime_1","UInt16",0.001,"Y",null,null,"设备1_读写D6090","设备0_读写D6090","设备2_读写D6090","设备3_读写D6090","设备4_读写D6090"]
["配料参数","2#最小时间","MinTime_2","UInt16",0.001,"Y",null,null,"设备1_读写D5090","设备0_读写D5090","设备2_读写D5090","设备3_读写D5090","设备4_读写D5090"]
["配料参数","3#最小时间","MinTime_3","UInt16",0.001,"Y",null,null,"设备1_读写D4090","设备0_读写D4090","设备2_读写D4090","设备3_读写D4090","设备4_读写D4090"]
["配料参数","4#最小时间","MinTime_4","UInt16",0.001,"Y",null,null,"设备1_读写D3090","设备0_读写D3090","设备2_读写D3090","设备3_读写D3090","设备4_读写D3090"]
["配料参数","5#最小时间","MinTime_5","UInt16",0.001,"Y",null,null,"设备1_读写R5090",null,"设备2_读写R5090",null,"设备4_读写R6090"]
["配料参数","6#最小时间","MinTime_6","UInt16",0.001,"Y",null,null,null,null,null,null,"设备4_读写R5090"]
["配料参数","1#稳重时间","StableTime_1","UInt16",0.1,"Y",null,null,"设备1_读写D2504","设备0_读写D2504","设备2_读写D2504","设备3_读写D2504","设备4_读写D2504"]
["配料参数","2#稳重时间","StableTime_2","UInt16",0.1,"Y",null,null,"设备1_读写D2505","设备0_读写D2505","设备2_读写D2505","设备3_读写D2505","设备4_读写D2505"]
["配料参数","3#稳重时间","StableTime_3","UInt16",0.1,"Y",null,null,"设备1_读写D2506","设备0_读写D2506","设备2_读写D2506","设备3_读写D2506","设备4_读写D2506"]
["配料参数","4#稳重时间","StableTime_4","UInt16",0.1,"Y",null,null,"设备1_读写D2507","设备0_读写D2507","设备2_读写D2507","设备3_读写D2507","设备4_读写D2507"]
["配料参数","5#稳重时间","StableTime_5","UInt16",0.1,"Y",null,null,"设备1_读写R2505",null,"设备2_读写R2505",null,"设备4_读写R2504"]
["配料参数","6#稳重时间","StableTime_6","UInt16",0.1,"Y",null,null,null,null,null,null,"设备4_读写R2505"]
["配料参数","1次料仓报警设定","BinAlarmSet_1","UInt16",null,"Y",null,null,"设备1_读写D3580","设备0_读写D3580","设备2_读写D3580","设备3_读写D3580","设备4_读写D3580"]
["配料参数","2次料仓报警设定","BinAlarmSet_2","UInt16",null,"Y",null,null,"设备1_读写D3582","设备0_读写D3582","设备2_读写D3582","设备3_读写D3582","设备4_读写D3582"]
["配料参数","3次料仓报警设定","BinAlarmSet_3","UInt16",null,"Y",null,null,"设备1_读写D3584","设备0_读写D3584","设备2_读写D3584","设备3_读写D3584","设备4_读写D3584"]
["配料参数","4次料仓报警设定","BinAlarmSet_4","UInt16",null,"Y",null,null,"设备1_读写D3586","设备0_读写D3586","设备2_读写D3586","设备3_读写D3586","设备4_读写D3586"]
["配料参数","5次料仓报警设定","BinAlarmSet_5","UInt16",null,"Y",null,null,"设备1_读写R3580",null,"设备2_读写R3580",null,"设备4_读写R3580"]
["配料参数","6次料仓报警设定","BinAlarmSet_6","UInt16",null,"Y",null,null,null,null,null,null,"设备4_读写R3582"]
["报警","No.1料仓缺料报警","IsErrorOfLack_1","bool",null,null,"Y",null,"设备1_读写M0501","设备0_读写M0500","设备2_读写M0501","设备3_读写M0500","设备4_读写M0500"]
["报警","No.2料仓缺料报警","IsErrorOfLack_2","bool",null,null,"Y",null,"设备1_读写M0502","设备0_读写M0501","设备2_读写M0502","设备3_读写M0501","设备4_读写M0501"]
["报警","No.3料仓缺料报警","IsErrorOfLack_3","bool",null,null,"Y",null,"设备1_读写M0503","设备0_读写M0502","设备2_读写M0503","设备3_读写M0502","设备4_读写M0502"]
["报警","No.4料仓缺料报警","IsErrorOfLack_4","bool",null,null,"Y",null,"设备1_读写S0500","设备0_读写M0503","设备2_读写S0500","设备3_读写M0503","设备4_读写M0503"]
["报警","No.5料仓缺料报警","IsErrorOfLack_5","bool",null,null,"Y",null,"设备1_读写S0501",null,"设备2_读写S0501",null,"设备4_读写S0500"]
["报警","No.6料仓缺料报警","IsErrorOfLack_6","bool",null,null,"Y",null,null,null,null,null,"设备4_读写S0501"]
["报警","No.1料斗加料异常","IsErrorOfAdd_1","bool",null,null,"Y",null,"设备1_读写M0511","设备0_读写M0510","设备2_读写M0511","设备3_读写M0510","设备4_读写M0510"]
["报警","No.2料斗加料异常","IsErrorOfAdd_2","bool",null,null,"Y",null,"设备1_读写M0512","设备0_读写M0511","设备2_读写M0512","设备3_读写M0511","设备4_读写M0511"]
["报警","No.3料斗加料异常","IsErrorOfAdd_3","bool",null,null,"Y",null,"设备1_读写M0513","设备0_读写M0512","设备2_读写M0513","设备3_读写M0512","设备4_读写M0512"]
["报警","No.4料斗加料异常","IsErrorOfAdd_4","bool",null,null,"Y",null,"设备1_读写S0510","设备0_读写M0513","设备2_读写S0510","设备3_读写M0513","设备4_读写M0513"]
["报警","No.5料斗加料异常","IsErrorOfAdd_5","bool",null,null,"Y",null,"设备1_读写S0511",null,"设备2_读写S0511",null,"设备4_读写S0510"]
["报警","No.6料斗加料异常","IsErrorOfAdd_6","bool",null,null,"Y",null,null,null,null,null,"设备4_读写S0511"]
["报警","螺杆缺料报警","IsErrorOfScrewLack","bool",null,null,"Y",null,"设备1_读写M0681","设备0_读写M0681","设备2_读写M0681","设备3_读写M0681","设备4_读写M0681"]
["报警","螺杆流量超偏差报警","IsErrorOfScrewFlow","bool",null,null,"Y",null,"设备1_读写M0684","设备0_读写M0684","设备2_读写M0684","设备3_读写M0684","设备4_读写M0684"]
["报警","搅拌电机故障","IsErrorOfBlender","bool",null,null,"Y",null,"设备1_只读X0002","设备0_只读X0002","设备2_只读X0002","设备3_只读X0002","设备4_只读X0002"]
["报警","急停开启","IsErrorOfScram","bool",null,null,"Y",null,"设备1_只读X0003","设备0_只读X0003","设备2_只读X0003","设备3_只读X0003","设备4_只读X0003"]
["报警","搅拌电机急停开启","IsErrorOfBlender2","bool",null,null,"Y",null,"设备1_只读X0004","设备0_只读X0004","设备2_只读X0004","设备3_只读X0004","设备4_只读X0004"]
["报警","搅拌电机未启动","IsErrorOfBlender3","bool",null,null,"Y",null,"设备1_读写M1300","设备0_读写M1300","设备2_读写M1300","设备3_读写M1300","设备4_读写M1300"]

{"sheet":"参数","index":5,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
["界面","描述","属性名","类型","放大","可写","报警","触发","HMI寄存器"]
["主界面","总流量设定","TotalFlowSetting","UInt16",0.1,"Y",null,null,"设备1_读写D3800"]
["主界面","总流量显示","TotalFlow","UInt16",0.1,null,null,null,"设备1_读写D3700"]
["主界面","总产量","TotalProduction","float",null,null,null,null,"设备1_读写D600"]
["主界面","码轮周长mm","WheelPerimeter","float",null,"Y",null,null,"设备1_读写R1014"]
["主界面","码轮脉冲","WheelPulse","float",null,"Y",null,null,"设备1_读写R1016"]
["主界面","平均密度","Density","float",null,"Y",null,null,"设备1_读写R1032"]
["主界面","边料不回收","IsRimNoRecycle","bool",null,"Y",null,null,"设备1_读写M0003"]
["主界面","边料kg/h","RimCharge","float",null,null,null,null,"设备1_读写R1308"]
["主界面","厚度um","Thickness","float",null,null,null,null,"设备1_读写R1040"]
["主界面","当前线速度m/min","CurrentVelocity","float",null,null,null,null,"设备1_读写R1050"]
["主界面","当前线速度设置m/min","CurrentVelocitySet","UInt16",0.1,"Y",null,null,"设备1_读写R1700"]
["主界面","吹膜宽度mm","TotalFilmWidth","float",null,"Y",null,null,"设备1_读写R1030"]
["主界面","切边mm","RimWidth","float",null,"Y",null,null,"设备1_读写R1204"]
["主界面","收卷宽度mm","ActFilmWidth","float",null,null,null,null,"设备1_读写R1206"]
["主界面","设定厚度um","SetThickness","float",null,"Y",null,null,"设备1_读写R1106"]
["主界面","理论速度m/min","TargetVelocity","float",null,null,null,null,"设备1_读写R1126"]
["主界面","内收卷当前m","ACurrentLen","float",null,null,null,null,"设备1_读写R1352"]
["主界面","内收卷当前kg","ACurrent","float",null,null,null,null,"设备1_读写R1236"]
["主界面","内收卷上卷kg","ALast","float",null,null,null,null,"设备1_读写R1602"]
["主界面","外收卷当前m","BCurrentLen","float",null,null,null,null,"设备1_读写R1354"]
["主界面","外收卷当前kg","BCurrent","float",null,null,null,null,"设备1_读写R1226"]
["主界面","外收卷上卷kg","BLast","float",null,null,null,null,"设备1_读写R1600"]
["主界面","内收卷清零","AClear","bool",null,"Y",null,null,"设备1_读写M0002"]
["主界面","外收卷清零","BClear","bool",null,"Y",null,null,"设备1_读写M0001"]