{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["参数","地址段映射","设备地址"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"参数","index":0,"n_rows":46,"n_cols":7,"rows_kept":46,"cut":false,"hidden":false,"merged":[]}
["界面","描述","属性名","类型","放大","可写","HMI寄存器"]
["风机控制","进风指示","IsInletAirOn","bool",null,"Y","设备0_Y(1)"]
["风机控制","进风运行频率(Hz)(自动调节)","InletAirFreq","uint16",0.1,null,"设备0_D(6120)"]
["风机控制","进风设定频率(Hz)","InletAirFreqSet","uint16",0.1,"Y","设备0_D(3200)"]
["风机控制","出风指示","IsOutletAirOn","bool",null,"Y","设备0_Y(2)"]
["风机控制","出风运行频率(Hz)","OutletAirFreq","uint16",0.1,null,"设备0_D(6220)"]
["风机控制","出风设定频率(Hz)","OutletAirFreqSet","uint16",0.1,"Y","设备0_D(592)"]
["风机控制","出风设定频率后通知","IsOutletAirFreqChanged","bool",null,"Y","设备0_M(99)"]
["风机控制","折径显示(mm)","FilmWidth","uint16",null,null,"设备0_D(668)"]
["风机控制","折径设定(mm)","FilmWidthSet","uint16",null,"Y","设备0_D(230)"]
["风机控制","折径设定后通知","IsFilmWidthChanged","bool",null,"Y","设备0_M(800)"]
["风机控制","误差校正","ErrorCorrection","int16",null,"Y","设备0_D(340)"]
["风机控制","IBC自动","IsIBCAuto","bool",null,"Y","设备0_M(659)"]
["膜泡校正","K1","K1","uint16",null,null,"设备0_D(1140)"]
["膜泡校正","K2","K2","uint16",null,null,"设备0_D(1142)"]
["膜泡校正","K3","K3","uint16",null,null,"设备0_D(1144)"]
["膜泡校正","L","L","float",null,"Y","设备0_D(250)"]
["膜泡校正","膜泡校正A","BubbleCorrA","float",null,null,"设备0_D(18)"]
["膜泡校正","膜泡校正B","BubbleCorrB","float",null,null,"设备0_D(28)"]
["膜泡校正","膜泡校正C","BubbleCorrC","float",null,null,"设备0_D(38)"]
["膜泡校正","膜泡校正R","BubbleCorrR","float",null,null,"设备0_D(102)"]
["IBC系统参数","采样周期","SampleInterval","uint16",0.1,"Y","设备0_D(300)"]
["IBC系统参数","区间1设置","Area1Set","uint16",null,"Y","设备0_D(304)"]
["IBC系统参数","区间1P","Area1P","uint16",null,"Y","设备0_D(1001)"]
["IBC系统参数","区间1I","Area1I","uint16",null,"Y","设备0_D(1002)"]
["IBC系统参数","区间1D","Area1D","uint16",null,"Y","设备0_D(1003)"]
["IBC系统参数","区间1DI","Area1DI","uint16",null,"Y","设备0_D(1004)"]
["IBC系统参数","调节系数","AdjustFactor","uint16",0.01,"Y","设备0_D(2550)"]
["IBC系统参数","PID结果","PIDResult","int16",null,"Y","设备0_D(2050)"]
["IBC系统参数","PID调节","PIDAdjust","int16",null,"Y","设备0_D(2052)"]
["IBC系统参数","进风速度","InletAirVelocity","uint16",null,"Y","设备0_D(710)"]
["IBC系统参数","出风速度","OutletAirVelocity","uint16",null,"Y","设备0_D(712)"]
["IBC系统参数2","区间2设置","Area2Set","uint16",null,"Y","设备0_D(306)"]
["IBC系统参数2","区间2P","Area2P","uint16",null,"Y","设备0_D(1201)"]
["IBC系统参数2","区间2I","Area2I","uint16",null,"Y","设备0_D(1202)"]
["IBC系统参数2","区间2D","Area2D","uint16",null,"Y","设备0_D(1203)"]
["IBC系统参数2","传感器1盲区","Sensor1DeadZone","float",null,"Y","设备0_D(420)"]
["IBC系统参数2","传感器2盲区","Sensor2DeadZone","float",null,"Y","设备0_D(430)"]
["IBC系统参数2","传感器3盲区","Sensor3DeadZone","float",null,"Y","设备0_D(440)"]
["IBC系统参数2","传感器1系数","Sensor1Factor","float",null,"Y","设备0_D(200)"]
["IBC系统参数2","传感器2系数","Sensor2Factor","float",null,"Y","设备0_D(400)"]
["IBC系统参数2","传感器3系数","Sensor3Factor","float",null,"Y","设备0_D(410)"]
["报警","进风变频故障报警","IsInletAirMotorError","bool",null,null,"设备0_X(10)"]
["报警","出风变频故障报警","IsOutletAirMotorError","bool",null,null,"设备0_X(11)"]
["报警","进风变频通讯报警","IsInletAirCommError","bool",null,null,"设备0_M(403)"]
["报警","出风变频通讯报警","IsOutletAirCommError","bool",null,null,"设备0_M(404)"]

{"sheet":"地址段映射","index":1,"n_rows":5,"n_cols":4,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
["PLC寄存器类型","PLC寄存器首地址","MB寄存器类型","MB寄存器首地址"]
["D",0,"[4区]输出寄存器",1]
["M",0,"[0区]输出继电器",1]
["Y",0,"[0区]输出继电器",64513]
["X",0,"[1区]输入继电器",63489]

{"sheet":"设备地址","index":2,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["设备序号","EP"]
[0,"192.168.50.30:502"]