{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["参数","收卷参数","地址段映射","设备地址"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"参数","index":0,"n_rows":67,"n_cols":7,"rows_kept":67,"cut":false,"hidden":false,"merged":[]}
["界面","描述","属性名","类型","放大","可写","HMI寄存器"]
["速度控制","设定速度(m/min)","VelocitySet","float",null,"Y","D(980)"]
["速度控制","速度确定(┷）","IsVelocityChanged","bool",null,"Y","M(650)"]
["速度控制","速度显示(m/min)","Velocity","float",null,null,"D(180)"]
["速度控制","上牵引电机电流(A)","Traction1Current","uint16",0.1,null,"D(1008)"]
["速度控制","上牵引开启显示","IsTraction1On","bool",null,null,"Y(0)"]
["速度控制","上牵引开启设置","IsTraction1OnSet","bool",null,"Y","M(580)"]
["速度控制","二牵引设定张力(kg)","Traction2TensionKgSet","uint16",0.1,"Y","D(6026)"]
["速度控制","二牵引实际张力(kg)","Traction2TensionKg","int16",0.1,null,"D(2254)"]
["速度控制","二牵引电机电流(A)","Traction2Current","uint16",0.1,null,"D(1108)"]
["速度控制","二牵引手动","IsTraction2Manual","bool",null,null,"M(651)"]
["速度控制","二牵引开启显示","IsTraction2On","bool",null,null,"Y(2)"]
["速度控制","二牵引开启设置","IsTraction2OnSet","bool",null,"Y","M(581)"]
["旋转塔","旋转塔正转","IsRotaryForw","bool",null,null,"Y(10)"]
["旋转塔","旋转塔反转","IsRotaryBackw","bool",null,null,"Y(45)"]
["旋转塔","旋转塔正向机械限位","IsRotaryForwLimit","bool",null,null,"X(32)"]
["旋转塔","旋转塔正转换向限位","IsRotaryForwTurn","bool",null,null,"X(30)"]
["旋转塔","旋转塔复位原点限位","IsRotaryOrgSign","bool",null,null,"X(27)"]
["旋转塔","旋转塔反转换向限位","IsRotaryBackwTurn","bool",null,null,"X(31)"]
["旋转塔","旋转塔反向机械限位","IsRotaryBackwLimit","bool",null,null,"X(33)"]
["旋转塔","旋转塔电机频率设定(Hz)","RotaryFreqSet","uint16",0.01,"Y","D(1380)"]
["旋转塔","旋转塔电机频率确定","IsRotaryFreqChanged","bool",null,"Y","M(190)"]
["旋转塔","旋转塔电机频率显示(Hz)","RotaryFreq","uint16",0.01,null,"D(1381)"]
["旋转塔","旋转塔电机电流(A)","RotaryCurrent","uint16",0.01,null,"D(1384)"]
["旋转塔","旋转塔复位指示","IsRotaryOrg","bool",null,"Y","M(414)"]
["旋转塔","旋转塔复位(┷）","RotaryOrg","bool",null,"Y","M(413)"]
["旋转塔","旋转塔开启指示","IsRotaryOn","bool",null,"Y","M(411)"]
["旋转塔","旋转塔开启(┷）","RotaryOn","bool",null,"Y","M(416)"]
["牵引","一牵引调试On","IsTraction1Debug","bool",null,"Y","M(656)"]
["牵引","一牵引辊筒直径","Traction1RollerD","float",null,"Y","D(5100)"]
["牵引","一牵引传动速比","Traction1GearRatio","float",null,"Y","D(5102)"]
["牵引","一牵引同步速度","Traction1SyncV","uint16",null,null,"D(114)"]
["牵引","一牵引实际速度","Traction1Velocity","uint16",null,null,"D(114)"]
["牵引","二牵引张力反馈","Traction2Tension","int16",null,null,"D(2400)"]
["牵引","二牵引张力设定","Traction2TensionSet","uint16",null,"Y","D(2250)"]
["牵引","二牵引增益设定","Traction2Gain","uint16",0.01,"Y","D(3080)"]
["牵引","二牵引积分时间","Traction2ITime","uint16",null,"Y","D(3004)"]
["牵引","二牵引调节系数","Traction2Factor","uint16",0.01,"Y","D(3050)"]
["牵引","二牵引辊筒直径","Traction2RollerD","float",null,"Y","D(5200)"]
["牵引","二牵引传动速比","Traction2GearRatio","float",null,"Y","D(5202)"]
["牵引","二牵引PID结果","Traction2PIDResult","int16",null,null,"D(3030)"]
["牵引","二牵引PID调节","Traction2PIDAdjust","int16",null,null,"D(3058)"]
["牵引","二牵引同步速度","Traction2SyncV","uint16",null,null,"D(5268)"]
["牵引","二牵引实际速度","Traction2Velocity","uint16",null,null,"D(5800)"]
["牵引","速度系数","VelocityFactor","float",null,"Y","D(5104)"]
["牵引","加减时间","AccDecTime","float",null,"Y","D(990)"]
["牵引","二牵引升降增益","Traction2LiftGain","uint16",0.01,"Y","D(3082)"]
["牵引","张力检测设定","TensionDetection","uint16",0.1,"Y","D(3860)"]
["收卷参数","收卷计米辊周长(mm)","WinderMeasurePerimeter","float",null,"Y","D(912)"]
["收卷参数","张力检测量程(kg)","TensionDetectionRange","uint16",0.1,"Y","D(2840)"]
["报警"," 主牵引风机过载报警！！！请检查(OFF)","IsError_Traction1Fan","bool",null,null,"X(3)"]
["报警"," 主牵引变频故障报警！！！请检查(ON)","IsError_Traction1VFD","bool",null,null,"M(480)"]
["报警"," 二牵引变频故障报警！！！请检查(ON)","IsError_Traction2VFD","bool",null,null,"M(481)"]
["报警"," 二牵引风机过载报警！！！请检查(OFF)","IsError_Traction2Fan","bool",null,null,"X(6)"]
["报警"," 旋转塔变频故障报警！！！请检查(ON)","IsError_RotaryVFD","bool",null,null,"M(484)"]
["报警"," 旋转塔风机过载报警！！！请检查(OFF)","IsError_RotaryFan","bool",null,null,"X(17)"]
["报警"," 二牵引拉线急停开启！！！请复位(OFF)","IsError_Traction2Scram","bool",null,null,"X(21)"]
["报警"," 电柜急停开启！！！请复位(OFF)","IsError_Scram","bool",null,null,"X(20)"]
["报警"," 主牵引拉线急停开启！！！请复位(OFF)","IsError_Traction1Scram","bool",null,null,"X(45)"]
["报警"," 客户急停开启！！！请复位(OFF)","IsError_CustomerScram","bool",null,null,"X(57)"]
["报警"," 旋转塔正转已到极限位！！！请检查(OFF)","IsError_RotaryForwLimit","bool",null,null,"X(32)"]
["报警"," 旋转塔反转已到极限位！！！请检查(OFF)","IsError_RotaryBackwLimit","bool",null,null,"X(33)"]
["报警"," 转塔正向极限锁定！！！请解除(ON)","IsError_RotaryForwLock","bool",null,null,"M(1202)"]
["报警"," 转塔反向极限锁定！！！请解除(ON)","IsError_RotaryBackwLock","bool",null,null,"M(1203)"]
["报警"," 一牵变频通讯故障！！！请检查(ON)","IsError_Traction1CommErr","bool",null,null,"M(142)"]
["报警"," 二牵变频通讯故障！！！请检查(ON)","IsError_Traction2CommErr","bool",null,null,"M(143)"]
[null," 旋转变频通讯故障！！！请检查(ON)","IsError_RotaryCommErr","bool",null,null,"M(146)"]

{"sheet":"收卷参数","index":1,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[]}
["界面","描述","属性名","类型","放大","可写","内收卷HMI寄存器","外收卷HMI寄存器"]
["收卷计量","收卷实际m","MeasureLen","uint32",null,null,"D(924)","D(916)"]
["收卷计量","收卷设定m","MeasureLenSet","uint32",null,"Y","D(936)","D(930)"]
["收卷计量","收卷预警m","MeasurePreWarning","uint32",null,"Y","D(942)","D(940)"]
["收卷计量","收卷计量关","MeasureStop","bool",null,"Y","M(901)","M(900)"]
["收卷计量","收卷计量清零(┷）","MeasureReset","bool",null,"Y","M(601)","M(600)"]
["手动操作","收卷翻转点动(┷）","TurnoverInching","bool",null,"Y","M(154)","M(150)"]
["手动操作","收卷切膜飞刀(┷）","CuttingFilm","bool",null,"Y","M(155)","M(151)"]
["手动操作","收卷翻转原点(┷）","TurnoverOrg","bool",null,"Y","M(156)","M(152)"]
["手动操作","收卷压臂平移(┷）","PressureArmOffset","bool",null,"Y","M(157)","M(153)"]
["收卷参数","收卷翻转上位等待(s)","TurnoverUpperWait","uint16",0.1,"Y","D(1620)","D(1720)"]
["收卷参数","收卷翻转原点延时(s)","TurnoverOrgDelay","uint16",0.1,"Y","D(1604)","D(1704)"]
["收卷参数","收卷翻转返回延时(s)","TurnoverBackDelay","uint16",0.1,"Y","D(1602)","D(1702)"]
["收卷参数","收卷锯齿切膜延时(s)","CuttingFilmDelay","uint16",0.1,"Y","D(1600)","D(1700)"]
["收卷参数","收卷锯齿切膜时间(s)","CuttingFilmElapsed","uint16",0.1,"Y","D(1601)","D(1701)"]
["收卷参数","收卷压臂返回时间(s)","PressureArmBackElapsed","uint16",0.1,"Y","D(1608)","D(1708)"]
["收卷参数","收卷气涨轴检测报警(s)","AirRollerCheck","uint16",0.1,"Y","D(1741)","D(1740)"]
["收卷参数","收卷一次平移时间(s)","OffsetElapsed","uint16",0.1,"Y","D(860)","D(864)"]
["收卷参数","收卷平移停顿时间(s)","ElapsedWait","uint16",0.1,"Y","D(862)","D(866)"]
["收卷参数","收卷接料限幅","TapeLimit","uint16",0.1,"Y","D(2570)","D(2572)"]
["速度控制","收卷设定张力(kg)","TensionKgSet","uint16",0.1,"Y","D(6027)","D(6028)"]
["速度控制","收卷实际张力(kg)","TensionKg","int16",0.1,null,"D(3336)","D(3356)"]
["速度控制","收卷电机电流(A)","Current","uint16",0.1,null,"D(1208)","D(1308)"]
["速度控制","收卷手动","IsManual","bool",null,"Y","M(652)","M(653)"]
["速度控制","收卷开启显示","IsOn","bool",null,null,"Y(4)","Y(6)"]
["速度控制","收卷开启设置","IsOnSet","bool",null,"Y","M(582)","M(583)"]
["牵引","收卷张力反馈","Tension","int16",null,null,"D(2500)","D(2600)"]
["牵引","收卷张力设定","TensionSet","uint16",null,"Y","D(3330)","D(3350)"]
["牵引","收卷增益设定","Gain","uint16",0.01,"Y","D(3180)","D(3280)"]
["牵引","收卷积分时间","ITime ","uint16",null,"Y","D(3104)","D(3204)"]
["牵引","收卷调节系数","Factor","uint16",0.01,"Y","D(3150)","D(3250)"]
["牵引","收卷辊筒直径","RollerD","float",null,"Y","D(5300)","D(5400)"]
["牵引","收卷传动速比","GearRatio","float",null,"Y","D(5302)","D(5402)"]
["牵引","收卷PID结果","PIDResult","int16",null,null,"D(3130)","D(3230)"]
["牵引","收卷PID调节","PIDAdjust","int16",null,null,"D(3158)","D(3258)"]
["牵引","收卷同步速度","SyncV","uint16",null,null,"D(5368)","D(5468)"]
["牵引","收卷实际速度","Velocity","uint16",null,null,"D(5802)","D(5804)"]
["牵引","收卷升降增益","LiftGain","uint16",0.01,"Y","D(3182)","D(3282)"]
["牵引","收卷速度补偿","VelocityComp","uint16",null,"Y","D(5668)","D(5688)"]
["报警","收卷变频故障报警！！！请检查(ON)","IsError_VFD","bool",null,null,"M(482)","M(483)"]
["报警","收卷风机过载报警！！！请检查(OFF)","IsError_Fan","bool",null,null,"X(11)","X(14)"]
["报警","收翻转刀架过载报警！！！请检查(OFF)","IsError_Turnover","bool",null,null,"X(67)","X(70)"]
["报警","收卷急停开启！！！请复位(OFF)","IsError_Scram","bool",null,null,"X(56)","X(44)"]
["报警","收卷换卷气涨轴检测未到位报警！！！请检查(ON)","IsError_AirRollerNoReady","bool",null,null,"M(443)","M(444)"]
["报警","收预警长度报警！！！请准备换卷(ON)","IsError_MeasurePreWarning","bool",null,null,"M(603)","M(602)"]
["报警","收卷换卷提醒报警！！！请注意安全(ON)","IsError_ChangeRoll","bool",null,null,"M(50)","M(51)"]
["报警","收卸料臂检测报警(ON)","IsError_UnloadArm","bool",null,null,"M(371)","M(370)"]
["报警","变频通讯故障！！！请检查(ON)","IsError_CommErr","bool",null,null,"M(144)","M(145)"]

{"sheet":"地址段映射","index":2,"n_rows":5,"n_cols":4,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
["PLC寄存器类型","PLC寄存器首地址","MB寄存器类型","MB寄存器首地址"]
["D",0,"[4区]输出寄存器",1]
["M",0,"[0区]输出继电器",1]
["Y",0,"[0区]输出继电器",64513]
["X",0,"[1区]输入继电器",63489]

{"sheet":"设备地址","index":3,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["设备序号","EP"]
[0,"192.168.50.40:502"]